{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["検索","データ","検索条件","建具の仕様・改修方法"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":7,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"検索","index":0,"n_rows":16,"n_cols":2,"rows_kept":16,"cut":false,"hidden":false,"merged":[[1,0,1,5],[15,1,15,4],[3,2,3,3],[5,2,5,3],[7,2,7,3],[9,2,9,3],[11,2,11,3],[13,2,13,3],[13,4,13,5],[3,4,3,5],[5,4,5,5],[7,4,7,5],[9,4,9,5],[11,4,11,5]]}
[]
["製品検索"]
[]
[null,"カテゴリ"]
[]
[null,"メーカー名"]
[]
[null,"対象製品番号"]
[]
[null,"製品名"]
[]
[null,"グレード"]
[]
[null,"建具の仕様・改修工法"]
[]
[null,"<最小中空層の厚さについて>\n・室外側から順に表記しています。\n・導入するガラスの中空層の厚さは、最小中空層の厚さ以上としてください。"]

{"sheet":"データ","index":1,"n_rows":1144,"n_cols":18,"rows_kept":1144,"cut":false,"hidden":true,"merged":[[0,0,0,4],[0,5,0,6],[0,7,0,10],[0,11,0,17]]}
["共通",null,null,null,null,"断熱材",null,"ガラス",null,null,null,"窓"]
["カテゴリ","メーカー名","対象製品番号","製品名","グレード","断熱材の種類","熱伝導率[W/(m･K)]","中空層の種類","最小中空層の厚さ_一層目","最小中空層の厚さ_二層目","アタッチメント","建具の仕様・改修工法","最小中空層の厚さ_一層目","最小中空層の厚さ_二層目","最小中空層の厚さ_三層目","最小中空層の厚さ_四層目","ガラス仕様","ガラス中空層の種類"]
["断熱材","株式会社アイシネン　アジア・パシフィック","DIAPA23PS3","アイシネンLDフォーム","D3","吹付け硬質ウレタンフォームA種３",3.7999999999999999E-2]
["断熱材","アキレス株式会社","DACHA31PU2","アキレスボードALN","D2","硬質ウレタンフォーム断熱材2種2号",2.4E-2]
["断熱材","アキレス株式会社","DACHA41PU2","アキレスボードAG","D2","硬質ウレタンフォーム断熱材2種2号",2.4E-2]
["断熱材","アキレス株式会社","DACHA51PU2","アキレスボードWAL-D","D2","硬質ウレタンフォーム断熱材2種2号",2.4E-2]
["断熱材","アキレス株式会社","DACH012PU1","キューワンボード","D1","硬質ウレタンフォーム断熱材2種2号",2.1000000000000001E-2]
["断熱材","アキレス株式会社","DACH022PU1","キューワンボードRZ","D1","硬質ウレタンフォーム断熱材2種2号",2.1000000000000001E-2]
["断熱材","アキレス株式会社","DACH013PU2","アキレスボードPE","D2","硬質ウレタンフォーム断熱材2種2号",2.4E-2]
["断熱材","アキレス株式会社","DACH063PU2","アキレスボードGFノンフロン(高密度)","D2","硬質ウレタンフォーム断熱材3種1号",2.4E-2]
["断熱材","アキレス株式会社","DACH073PU2","ニューハウスボード","D2","硬質ウレタンフォーム断熱材2種2号",2.4E-2]
["断熱材","アキレス株式会社","DACHA13PU2","アキレス準不燃NDパネル","D2","硬質ウレタンフォーム断熱材（2種） PUF2.2A",2.4E-2]
["断熱材","アキレス株式会社","DACHA23PU2","アキレス準不燃NDパネル　防水石膏タイプ","D2","硬質ウレタンフォーム断熱材（2種） PUF2.2A",2.4E-2]
["断熱材","アキレス株式会社","DACHA33PU2","アキレスHCパネル","D2","硬質ウレタンフォーム断熱材（2種） PUF2.2A",2.4E-2]
["断熱材","アキレス株式会社","DACHF13PS2","アキレスエアロンFR-FO","D2","建築物用吹付け硬質ウレタンフォーム（A種１H） NF1H",2.5999999999999999E-2]
["断熱材","アキレス株式会社","DACH013PS3","アキレスKHフォーム","D3","吹付け硬質ウレタンフォームA種３",0.04]
["断熱材","旭化成建材株式会社","DAKKN11PH1","ネオマフォーム","D1","フェノールフォーム断熱材１種２号CII",0.02]
["断熱材","旭化成建材株式会社","DAKKN31PH1","ネオマゼウス","D1","フェノールフォーム断熱材１種２号EII",1.7999999999999999E-2]
["断熱材","旭ファイバーグラス株式会社","DAFG012PU1","AFボード(KS)","D1","A種硬質ウレタンフォーム保温板２種２号",2.1000000000000001E-2]
["断熱材","旭ファイバーグラス株式会社","DAFGA12GW2","アクリアウールα36K","D2","高性能グラスウール断熱材４０Ｋ相当",3.2000000000000001E-2]
["断熱材","旭ファイバーグラス株式会社","DAFGA22GW2","アクリアUボードピンレスα36K","D2","高性能グラスウール断熱材４０Ｋ相当",3.2000000000000001E-2]
["断熱材","旭ファイバーグラス株式会社","DAFGD31GW2","アクリアα36K","D2","グラスウール断熱材（高性能品）GWHG36-32",3.2000000000000001E-2]
["断熱材","旭ファイバーグラス株式会社","DAFG011GW3","アクリアマット16K","D3","高性能グラスウール断熱材１６Ｋ相当",3.7999999999999999E-2]
["断熱材","旭ファイバーグラス株式会社","DAFG012GW3","アクリアネクスト14K","D3","高性能グラスウール断熱材１４Ｋ",3.7999999999999999E-2]
["断熱材","旭ファイバーグラス株式会社","DAFG021GW3","アクリアウール16K","D3","高性能グラスウール断熱材１６Ｋ相当",3.7999999999999999E-2]
["断熱材","旭ファイバーグラス株式会社","DAFG022GW3","アクリアマット14K","D3","高性能グラスウール断熱材１４Ｋ",3.7999999999999999E-2]
["断熱材","旭ファイバーグラス株式会社","DAFG031GW3","アクリアウール24K","D3","高性能グラスウール断熱材２４Ｋ相当",3.5999999999999997E-2]
["断熱材","旭ファイバーグラス株式会社","DAFG032GW3","アクリアサンカット14K","D3","高性能グラスウール断熱材１４Ｋ",3.7999999999999999E-2]
["断熱材","旭ファイバーグラス株式会社","DAFG041GW3","アクリアサンカット24K","D3","高性能グラスウール断熱材２４Ｋ相当",3.5999999999999997E-2]
["断熱材","旭ファイバーグラス株式会社","DAFG051GW3","アクリアUボードピンレス24K","D3","高性能グラスウール断熱材２４Ｋ相当",3.5999999999999997E-2]
["断熱材","旭ファイバーグラス株式会社","DAFG061GW3","アクリアUボードNT24K","D3","高性能グラスウール断熱材２４Ｋ相当",3.5999999999999997E-2]
["断熱材","旭ファイバーグラス株式会社","DAFG071GW3","アクリアUボードピンレス32K","D3","高性能グラスウール断熱材３２Ｋ相当",3.5000000000000003E-2]
["断熱材","旭ファイバーグラス株式会社","DAFG081GW3","アクリアUボードNT32K","D3","高性能グラスウール断熱材３２Ｋ相当",3.5000000000000003E-2]
["断熱材","旭ファイバーグラス株式会社","DAFGA11GW3","アクリアネクストα20K","D3","高性能グラスウール断熱材４０Ｋ相当",3.4000000000000002E-2]
["断熱材","旭ファイバーグラス株式会社","DAFGA21GW3","アクリアマットα20K","D3","高性能グラスウール断熱材４０Ｋ相当",3.4000000000000002E-2]
["断熱材","旭ファイバーグラス株式会社","DAFGA31GW3","アクリアウールα20K","D3","高性能グラスウール断熱材４０Ｋ相当",3.4000000000000002E-2]
["断熱材","旭ファイバーグラス株式会社","DAFGB21GW3","マットエース24","D3","グラスウール断熱材　２４Ｋ（ＧＷ２４－３８）",3.7999999999999999E-2]
["断熱材","旭ファイバーグラス株式会社","DAFGB31GW3","住宅用グラスウール断熱材P1","D3","グラスウール断熱材　２４Ｋ（ＧＷ２４－３８）",3.7999999999999999E-2]
["断熱材","旭ファイバーグラス株式会社","DAFGB41GW3","住宅用高性能グラスウール断熱材P2","D3","高性能グラスウール断熱材　１６Ｋ（ＧＷＨＧ１６－３８）",3.7999999999999999E-2]
["断熱材","旭ファイバーグラス株式会社","DAFGB51GW3","住宅用高性能グラスウール断熱材P3","D3","高性能グラスウール断熱材　１４Ｋ（ＧＷＨＧ１４－３８）",3.7999999999999999E-2]
["断熱材","旭ファイバーグラス株式会社","DAFGB61GW3","住宅用高性能グラスウール断熱材P4","D3","高性能グラスウール断熱材　２４Ｋ（ＧＷＨＧ２４－３６）",3.5999999999999997E-2]
["断熱材","旭ファイバーグラス株式会社","DAFGB71GW3","住宅用高性能グラスウール断熱材P5","D3","高性能グラスウール断熱材　２０Ｋ（ＧＷＨＧ２０－３６）",3.5999999999999997E-2]
["断熱材","旭ファイバーグラス株式会社","DAFGD01GW3","アクリアマット16K","D3","グラスウール断熱材（高性能品）GWHG16-37",3.6999999999999998E-2]
["断熱材","旭ファイバーグラス株式会社","DAFGD11GW3","アクリアマット24K","D3","グラスウール断熱材（高性能品）GWHG24-34",3.4000000000000002E-2]
["断熱材","旭ファイバーグラス株式会社","DAFGD21GW3","アクリアα20K","D3","グラスウール断熱材（高性能品）GWHG20-34",3.4000000000000002E-2]
["断熱材","旭ファイバーグラス株式会社","DAFG044GB4","(北海道向け)ニューブローエース18K","D4","天井断熱工事用吹込みグラスウール１８Ｋ",5.1999999999999998E-2]
["断熱材","旭ファイバーグラス株式会社","DAFGE13GB4","アクリアEブロー　10K","D4","吹込み用繊維質断熱材　天井用",5.1999999999999998E-2]
["断熱材","旭有機材株式会社","DAOCA43PS2","ゼロフロンER-X","D2","吹付け硬質ウレタンフォームA種１H",2.5999999999999999E-2]
["断熱材","旭有機材株式会社","DAOCA23PS3","APS-NZ","D3","吹付け硬質ウレタンフォームA種１",3.4000000000000002E-2]
["断熱材","旭有機材株式会社","DAOCA33PS3","ゼロフロンフィット","D3","吹付け硬質ウレタンフォームA種３",0.04]
["断熱材","株式会社アップルゲートジャパン","DS12A13CB3","アップルゲートセルロース断熱材","D3","吹付け用セルロースファイバー４５Ｋ",4.1000000000000002E-2]
["断熱材","イビデン樹脂株式会社","DIBDA13EP3","アイフォームG ネダレス用","D3","ビーズ法ポリスチレンフォーム1号",3.4000000000000002E-2]
["断熱材","イビデン樹脂株式会社","DIBDA23EP3","アイフォームG ネダ用","D3","ビーズ法ポリスチレンフォーム1号",3.4000000000000002E-2]
["断熱材","岩倉化学工業株式会社","DE01011EP3","セルボード","D3","A種ビーズ法ポリスチレンフォーム保温板特号",3.4000000000000002E-2]
["断熱材","ウッドファイバー株式会社","DWODA11IB3","ウッドファイバーLD-B","D3","インシュレーションファイバー断熱材40K",0.04]
["断熱材","ウッドファイバー株式会社","DWODA21IB3","ウッドファイバーLD-B","D3","インシュレーションファイバー断熱材55K",0.04]
["断熱材","ウッドファイバー株式会社","DWODA31IB3","ウッドファイバーLD-B","D3","インシュレーションファイバー断熱材60K",0.04]
["断熱材","ウッドファイバー株式会社","DWODA41IB3","ウッドファイバーLD-B","D3","インシュレーションファイバー断熱材80K",0.04]
["断熱材","ウッドファイバー株式会社","DWODA51IB3","ウッドファイバーLD","D3","インシュレーションファイバー断熱材40K",0.04]
["断熱材","ウッドファイバー株式会社","DWODA61IB3","ウッドファイバーLD","D3","インシュレーションファイバー断熱材55K",0.04]
["断熱材","ウッドファイバー株式会社","DWODA71IB3","ウッドファイバーLD","D3","インシュレーションファイバー断熱材60K",0.04]
["断熱材","ウッドファイバー株式会社","DWODA81IB3","ウッドファイバーLD","D3","インシュレーションファイバー断熱材80K",0.04]
["断熱材","エコネクストネット株式会社","DECOA11CB3","チャフパック","D3","吹込み用セルロースファイバー４５Ｋ",0.04]
["断熱材","株式会社FPコーポレーション","DS50011PU2","ﾗｸﾃｨC","D2","A種硬質ウレタンフォーム保温板２種２号",2.4E-2]
["断熱材","エンデバーハウス株式会社","DEHS015MI3","パーフェクトバリア　ロールタイプ13K R2.7","D3","その他",3.9E-2]
["断熱材","エンデバーハウス株式会社","DEHS025MI3","パーフェクトバリア　ボードタイプ30K R2.7","D3","その他",3.5000000000000003E-2]
["断熱材","エンデバーハウス株式会社","DEHSB15MI3","パーフェクトバリア　壁・屋根用ボードタイプ","D3","その他",3.5000000000000003E-2]
["断熱材","エンデバーハウス株式会社","DEHSP15MI3","パーフェクトバリア　ロールタイプ13K","D3","その他",3.9E-2]
["断熱材","エンデバーハウス株式会社","DEHSP25MI3","パーフェクトバリア　ロールタイプ13K耳付","D3","その他",3.9E-2]
["断熱材","エンデバーハウス株式会社","DEHSP35MI3","パーフェクトバリア　床用ボードタイプ","D3","その他",3.5000000000000003E-2]
["断熱材","エンデバーハウス株式会社","DEHSP45MI3","パーフェクトバリア　横裂サイドスリットタイプ","D3","その他",3.7999999999999999E-2]
["断熱材","王子製袋株式会社","DOJIA14CB3","ダンパック","D3","天井断熱工事用吹込みセルローズファイバー２５Ｋ",0.04]
["断熱材","王子製袋株式会社","DOJIA21CB3","ダンパック","D3","吹付け用セルロースファイバー４０Ｋ",0.04]
["断熱材","王子製袋株式会社","DOJIA31CB3","ダンパック","D3","吹込み用セルロースファイバー５０Ｋ",0.04]
["断熱材","王子製袋株式会社","DOJIA41CB3","チャフパック","D3","吹付け用セルロースファイバー４５Ｋ",0.04]
["断熱材","株式会社大西コルク工業所","DE50A11PE3","オーボード　3号","D3","ビーズ法ポリスチレンフォーム断熱材",3.7999999999999999E-2]
["断熱材","株式会社大西コルク工業所","DE50A21PE3","オーボード　4号","D3","ビーズ法ポリスチレンフォーム断熱材",4.1000000000000002E-2]
["断熱材","株式会社沖縄敷物商会","DT27011TM3","スタイロ畳GIIIタイプ　25","D3","建材畳III型５０mm厚２５",4.1000000000000002E-2]
["断熱材","株式会社沖縄敷物商会","DT27021TM3","スタイロ畳GIIタイプ　25","D3","建材畳II型５０mm厚２５",4.1000000000000002E-2]
["断熱材","株式会社沖縄敷物商会","DT27031TM3","スタイロ畳GIIタイプ　30","D3","建材畳II型５０mm厚３０",3.9E-2]
["断熱材","株式会社OKUTA","D013C13CB3","EMセルロースファイバー","D3","吹込み用セルロースファイバー５５Ｋ",4.1000000000000002E-2]
["断熱材","音熱環境開発株式会社","DONKD11RW3","イージーラメラ　ロックウール 80K","D3","ロックウール断熱材（ボード）",3.5999999999999997E-2]
["断熱材","音熱環境開発株式会社","DONKD21RW3","イージーラメラ　ロックウール 140K","D3","ロックウール断熱材（ボード）",3.5999999999999997E-2]
["断熱材","株式会社オーパス","DS83011CB3","ファイバーエース","D3","吹込み用セルロースファイバー５５Ｋ",0.04]
["断熱材","株式会社オーパス","DS83021CB3","ファイバーエース","D3","吹込み用セルロースファイバー２５Ｋ",0.04]
["断熱材","金山化成株式会社","DE40011EP3","SKフォーム　トクゴウボード","D3","A種ビーズ法ポリスチレンフォーム保温板特号",3.4000000000000002E-2]
["断熱材","金山化成株式会社","DE40012EP3","SKフォーム　N40","D3","A種ビーズ法ポリスチレンフォーム保温板４号",3.7999999999999999E-2]
["断熱材","金山化成株式会社","DE40021EP3","SKフォーム　3ゴウボード","D3","A種ビーズ法ポリスチレンフォーム保温板３号",0.04]
["断熱材","金山化成株式会社","DE40022EP3","ドライビットボード","D3","A種ビーズ法ポリスチレンフォーム保温板４号",0.04]
["断熱材","金山化成株式会社","DE40A11EP3","SKF JIS9521 1ゴウ","D3","ビーズ法ポリスチレンフォーム断熱材１号",3.4000000000000002E-2]
["断熱材","金山化成株式会社","DE40A21EP3","SKF JIS9521 2ゴウ","D3","ビーズ法ポリスチレンフォーム断熱材２号",3.5999999999999997E-2]
["断熱材","金山化成株式会社","DE40A31EP3","SKF JIS9521 3ゴウ","D3","ビーズ法ポリスチレンフォーム断熱材３号",3.7999999999999999E-2]
["断熱材","金山化成株式会社","DE40A41EP3","SKF JIS9521 4ゴウ","D3","ビーズ法ポリスチレンフォーム断熱材４号",4.1000000000000002E-2]
["断熱材","金山化成株式会社","DE40T12EP3","ターマイトバリアフォーム","D3","ビーズ法ポリスチレンフォーム保温材特号",3.4000000000000002E-2]
["断熱材","株式会社カネカ","DKNK011XP2","カネライトフォームスーパーE-III","D2","押出法ポリスチレンフォーム断熱材３種",2.8000000000000001E-2]
["断熱材","株式会社カネカ","DKNK041XP2","カネライトオメガE-III","D2","押出法ポリスチレンフォーム断熱材３種",2.8000000000000001E-2]
["断熱材","株式会社カネカ","DKNKA11XP2","カネライトフォームスーパーEX","D2","押出法ポリスチレンフォーム断熱材３種ｂＣ",2.4E-2]
["断熱材","株式会社カネカ","DKNKA71XP2","カネライトフォームスーパーE-BK","D2","押出法ポリスチレンフォーム断熱材３種ｂＡ",2.8000000000000001E-2]
["断熱材","株式会社カネカ","DKNK021XP3","カネライトフォームスーパーE-II","D3","押出法ポリスチレンフォーム断熱材２種",3.4000000000000002E-2]
["断熱材","株式会社カネカ","DKNK051XP3","カネライトオメガE-II","D3","押出法ポリスチレンフォーム断熱材２種",3.4000000000000002E-2]
["断熱材","株式会社カネカ","DKNKA31XP3","カネライトフォームスーパーE-I","D3","押出法ポリスチレンフォーム断熱材１種ｂＣ",3.5999999999999997E-2]
["断熱材","株式会社カネカ","DKNKA61XP3","カネライトオメガE-I","D3","押出法ポリスチレンフォーム断熱材１種ｂＣ",3.5999999999999997E-2]
["断熱材","株式会社兼久","DS86A73CB3","コンファイブ","D3","吹込み用繊維質断熱材",3.6999999999999998E-2]
["断熱材","クナウフ・インシュレーション合同会社","DKUFE11GW3","エコバット 16K","D3","グラスウール断熱材 高性能品 GWHG16-38",3.7999999999999999E-2]
["断熱材","クナウフ・インシュレーション合同会社","DKUFE21GW3","エコバット 24K","D3","グラスウール断熱材 高性能品 GWHG24-36",3.5999999999999997E-2]
["断熱材","クナウフ・インシュレーション合同会社","DKUFS21GW3","SUPAFIL 屋根･床･壁用","D3","吹込み用グラスウール断熱材 LFGW2636",3.5999999999999997E-2]
["断熱材","クナウフ・インシュレーション合同会社","DKUFS14GB4","SUPAFIL 天井用","D4","吹込み用グラスウール断熱材　天井用　　LFGW1351",5.0999999999999997E-2]
["断熱材","倉敷紡績株式会社","DKRBA41PU1","クランゼロボード","D1","硬質ウレタンフォーム断熱材２種２号D",2.1000000000000001E-2]
["断熱材","倉敷紡績株式会社","DKRBA11PU2","クランボードP","D2","硬質ウレタンフォーム断熱材２種２号A",2.4E-2]
["断熱材","倉敷紡績株式会社","DKRBA21PU2","クランボードL","D2","硬質ウレタンフォーム断熱材２種２号A",2.4E-2]
["断熱材","倉敷紡績株式会社","DKRBA31PU2","クランボードAP","D2","硬質ウレタンフォーム断熱材２種２号A",2.4E-2]
["断熱材","倉敷紡績株式会社","DKRBB23PS2","エアクララ(HR340NSG-L-F)","D2","吹付け硬質ウレタンフォームＡ種１H",2.5999999999999999E-2]
["断熱材","倉敷紡績株式会社","DKRB013PS3","ｿﾌﾃｨｾﾙONE","D3","吹付け硬質ウレタンフォームA種３",0.04]
["断熱材","有限会社齋藤製畳","DT07011TM3","カネライト畳","D3","建材畳II型５０mm厚３０",3.9E-2]
["断熱材","有限会社齋藤製畳","DT07021TM3","カネライト畳","D3","建材畳II型５０mm厚２５",4.1000000000000002E-2]
["断熱材","有限会社齋藤製畳","DT07031TM3","カネライト畳","D3","建材畳II型５５mm厚３５",3.7999999999999999E-2]
["断熱材","有限会社齋藤製畳","DT07041TM3","カネライト畳","D3","建材畳II型５５mm厚３０",0.04]
["断熱材","有限会社齋藤製畳","DT07051TM3","カネライト畳","D3","建材畳III型５０mm厚２５",4.1000000000000002E-2]
["断熱材","有限会社齋藤製畳","DT07061TM3","カネライト畳","D3","建材畳III型５５mm厚３０",0.04]
["断熱材","株式会社酒井寅雄商店","DT04011TM3","スタイロ畳　酒井寅雄商店　建材畳床II型-50","D3","建材畳II型５０mm厚３０",3.9E-2]
["断熱材","株式会社酒井寅雄商店","DT04021TM3","スタイロ畳　酒井寅雄商店　建材畳床II型-55","D3","建材畳II型５５mm厚３５",3.7999999999999999E-2]
["断熱材","株式会社酒井寅雄商店","DT04031TM3","スタイロ畳　酒井寅雄商店　建材畳床III型-50","D3","建材畳III型５０mm厚２５",4.1000000000000002E-2]
["断熱材","株式会社酒井寅雄商店","DT04041TM3","スタイロ畳　酒井寅雄商店　建材畳床III型-55","D3","建材畳III型５５mm厚３０",0.04]
["断熱材","三昌フォームテック株式会社","DE29012EP3","YSKボード　1号","D3","ビーズ法ポリスチレンフォーム断熱材　1号",3.4000000000000002E-2]
["断熱材","三昌フォームテック株式会社","DE29022EP3","YSKボード　2号","D3","ビーズ法ポリスチレンフォーム断熱材　2号",3.5000000000000003E-2]
["断熱材","三昌フォームテック株式会社","DE29032EP3","YSKボード　3号","D3","ビーズ法ポリスチレンフォーム断熱材　3号",3.5999999999999997E-2]
["断熱材","三昌フォームテック株式会社","DE29042EP3","YSKボード　4号","D3","ビーズ法ポリスチレンフォーム断熱材　4号",3.7999999999999999E-2]
["断熱材","三昌フォームテック株式会社","DE29A32EP3","ネダフォーム","D3","ビーズ法ポリスチレンフォーム断熱材　2号",3.5999999999999997E-2]
["断熱材","株式会社JSP","DJSPA61XP1","ミラフォームラムダ","D1","押出法ポリスチレンフォーム断熱材　３種ａＤ",2.1999999999999999E-2]
["断熱材","株式会社JSP","DJSPA31XP2","ミラフォームMKS","D2","押出法ポリスチレンフォーム断熱材　３種ｂＡ",2.8000000000000001E-2]
["断熱材","株式会社JSP","DJSPA41XP2","ミラフォームM2RS","D2","押出法ポリスチレンフォーム断熱材　３種ｂＡ",2.8000000000000001E-2]
["断熱材","株式会社JSP","DJSPA11XP3","ミラフォームM1F","D3","押出法ポリスチレンフォーム断熱材　１種ｂＣ",3.5999999999999997E-2]
["断熱材","株式会社JSP","DJSPA21XP3","ミラフォームM2F","D3","押出法ポリスチレンフォーム断熱材　２種ｂＡ",3.4000000000000002E-2]
["断熱材","株式会社JSP","DJSPA51XP3","ミラフォームMTS","D3","押出法ポリスチレンフォーム断熱材　１種ｂＣ",3.5999999999999997E-2]
["断熱材","JFEロックファイバー株式会社","DJFE011RW3","アムマット　厚さ 55mm","D3","ロックウール断熱材（マット）",3.7999999999999999E-2]
["断熱材","JFEロックファイバー株式会社","DJFE021RW3","アムマット　厚さ 77mm","D3","ロックウール断熱材（マット）",3.7999999999999999E-2]
["断熱材","JFEロックファイバー株式会社","DJFE031RW3","アムマット　厚さ 92mm","D3","ロックウール断熱材（マット）",3.7999999999999999E-2]
["断熱材","JFEロックファイバー株式会社","DJFE041RW3","アムマット　厚さ 100mm","D3","ロックウール断熱材（マット）",3.7999999999999999E-2]
["断熱材","JFEロックファイバー株式会社","DJFE051RW3","アムマット　厚さ 105mm","D3","ロックウール断熱材（マット）",3.7999999999999999E-2]
["断熱材","JFEロックファイバー株式会社","DJFE061RW3","アムマットプレミアム　厚さ 92mm","D3","ロックウール断熱材（マット）",3.7999999999999999E-2]
["断熱材","JFEロックファイバー株式会社","DJFE071RW3","アムマットプレミアム　厚さ 105mm","D3","ロックウール断熱材（マット）",3.7999999999999999E-2]
["断熱材","JFEロックファイバー株式会社","DJFEC11RW3","アムマット　厚さ 85mm　(RWMA)","D3","ロックウール断熱材（マット）",3.7999999999999999E-2]
["断熱材","JFEロックファイバー株式会社","DJFEC21RW3","アムマット　厚さ 140mm　(RWMA)","D3","ロックウール断熱材（マット）",3.7999999999999999E-2]
["断熱材","JFEロックファイバー株式会社","DJFEC31RW3","アムマット　厚さ 155mm　(RWMA)","D3","ロックウール断熱材（マット）",3.7999999999999999E-2]
["断熱材","JFEロックファイバー株式会社","DJFEC41RW3","アムマットプレミアム　厚さ 140mm　(RWMA)","D3","ロックウール断熱材（マット）",3.7999999999999999E-2]
["断熱材","JFEロックファイバー株式会社","DJFEC51RW3","アムマットプレミアム　厚さ 155mm　(RWMA)","D3","ロックウール断熱材（マット）",3.7999999999999999E-2]
["断熱材","株式会社ジョイ・コス","DJOYJ13PU2","ジョイ・コスパネル(炭化コルクタイプ)","D2","A種硬質ウレタンフォーム保温板２種3号",2.5000000000000001E-2]
["断熱材","株式会社ジョイ・コス","DJOYJ23PU2","ジョイ・コスパネル(ベニヤタイプ)","D2","A種硬質ウレタンフォーム保温板２種3号",2.5000000000000001E-2]
["断熱材","積水化学工業株式会社","DSKK012PH1","フェノバボードJ","D1","A種フェノールフォーム保温板３種１号",1.9E-2]
["断熱材","積水化学工業株式会社","DSKK022PH1","フェノバボード","D1","A種フェノールフォーム保温板１種２号",1.9E-2]
["断熱材","積水ソフランウイズ株式会社","DSLWA23PS2","ソフラン-R　LSP-BP3","D2","建築物断熱用吹付け硬質ウレタンフォームA種1H",2.5999999999999999E-2]
["断熱材","積水ソフランウイズ株式会社","DSLWA13PS3","ソフラン-R　ウイズフォーム","D3","吹付け硬質ウレタンフォームA種３",0.04]
["断熱材","タクミ建設株式会社","DWOLV15MI3","バージンウール呼吸性防音断熱材","D3","その他",3.7999999999999999E-2]
["断熱材","田島ルーフィング株式会社","DTAJA12PU2","ギルフォーム25S","D2","A種硬質ウレタンフォーム保温板２種１号",2.3E-2]
["断熱材","田島ルーフィング株式会社","DTAJA22PU2","ギルフォーム30S","D2","A種硬質ウレタンフォーム保温板２種１号",2.3E-2]
["断熱材","田島ルーフィング株式会社","DTAJA32PU2","ギルフォーム35S","D2","A種硬質ウレタンフォーム保温板２種１号",2.3E-2]
["断熱材","田島ルーフィング株式会社","DTAJA42PU2","ギルフォーム40S","D2","A種硬質ウレタンフォーム保温板２種１号",2.3E-2]
["断熱材","田島ルーフィング株式会社","DTAJA52PU2","ギルフォーム50S","D2","A種硬質ウレタンフォーム保温板２種１号",2.3E-2]
["断熱材","田島ルーフィング株式会社","DTAJA62PU2","ギルフォーム60S","D2","A種硬質ウレタンフォーム保温板２種１号",2.3E-2]
["断熱材","田島ルーフィング株式会社","DTAJB12PU2","VTボード25","D2","A種硬質ウレタンフォーム保温板２種１号",2.3E-2]
["断熱材","田島ルーフィング株式会社","DTAJB22PU2","VTボード30","D2","A種硬質ウレタンフォーム保温板２種１号",2.3E-2]
["断熱材","田島ルーフィング株式会社","DTAJB32PU2","VTボード35","D2","A種硬質ウレタンフォーム保温板２種１号",2.3E-2]
["断熱材","田島ルーフィング株式会社","DTAJB42PU2","VTボード40","D2","A種硬質ウレタンフォーム保温板２種１号",2.3E-2]
["断熱材","田島ルーフィング株式会社","DTAJB52PU2","VTボード50","D2","A種硬質ウレタンフォーム保温板２種１号",2.3E-2]
["断熱材","田島ルーフィング株式会社","DTAJC12PU2","GIボードW25","D2","A種硬質ウレタンフォーム保温板２種１号",2.3E-2]
["断熱材","田島ルーフィング株式会社","DTAJC22PU2","GIボードW30","D2","A種硬質ウレタンフォーム保温板２種１号",2.3E-2]
["断熱材","田島ルーフィング株式会社","DTAJC32PU2","GIボードW35","D2","A種硬質ウレタンフォーム保温板２種１号",2.3E-2]
["断熱材","田島ルーフィング株式会社","DTAJC42PU2","GIボードW40","D2","A種硬質ウレタンフォーム保温板２種１号",2.3E-2]
["断熱材","田島ルーフィング株式会社","DTAJC52PU2","GIボードW50","D2","A種硬質ウレタンフォーム保温板２種１号",2.3E-2]
["断熱材","田島ルーフィング株式会社","DTAJD12PU2","ギルフォーム25W","D2","A種硬質ウレタンフォーム保温板２種１号",2.3E-2]
["断熱材","田島ルーフィング株式会社","DTAJD22PU2","ギルフォーム30W","D2","A種硬質ウレタンフォーム保温板２種１号",2.3E-2]
["断熱材","田島ルーフィング株式会社","DTAJD32PU2","ギルフォーム35W","D2","A種硬質ウレタンフォーム保温板２種１号",2.3E-2]
["断熱材","田島ルーフィング株式会社","DTAJD42PU2","ギルフォーム40W","D2","A種硬質ウレタンフォーム保温板２種１号",2.3E-2]
["断熱材","田島ルーフィング株式会社","DTAJD52PU2","ギルフォーム50W","D2","A種硬質ウレタンフォーム保温板２種１号",2.3E-2]
["断熱材","田島ルーフィング株式会社","DTAJD62PU2","ギルフォーム60W","D2","A種硬質ウレタンフォーム保温板２種１号",2.3E-2]
["断熱材","龍野コルク工業株式会社","DTCKE43EP3","e-Form　SUPER　E4","D3","Ａ種ビーズ法ポリスチレンフォーム保温材保温板　４号",3.3000000000000002E-2]
["断熱材","ダイナガ化成株式会社","DE47A11EP3","スノーフォーム断熱材1号","D3","発泡プラスチック断熱材　ビーズ法ポリスチレンフォーム断熱材　1号",3.4000000000000002E-2]
["断熱材","ダイナガ化成株式会社","DE47A21EP3","スノーフォーム断熱材1号OP","D3","発泡プラスチック断熱材　ビーズ法ポリスチレンフォーム断熱材1号",3.4000000000000002E-2]
["断熱材","ダイナガ化成株式会社","DE47A31EP3","スノーフォーム断熱材3号","D3","発泡プラスチック断熱材　ビーズ法ポリスチレンフォーム断熱材3号",3.7999999999999999E-2]
["断熱材","ダイナガ化成株式会社","DE47A41EP3","スノーフォーム断熱材3号OP","D3","発泡プラスチック断熱材　ビーズ法ポリスチレンフォーム断熱材3号",3.7999999999999999E-2]
["断熱材","ダイナガ化成株式会社","DE47A51EP3","スノーフォーム断熱材4号","D3","発泡プラスチック断熱材　ビーズ法ポリスチレンフォーム断熱材4号",4.1000000000000002E-2]
["断熱材","ダイナガ化成株式会社","DE47A61EP3","スノーフォーム断熱材4号OP","D3","発泡プラスチック断熱材　ビーズ法ポリスチレンフォーム断熱材4号",4.1000000000000002E-2]
["断熱材","チヨダウーテ株式会社","DTIYE11GW3","アースウール16K","D3","グラスウール断熱材高性能製品　HG16-38",3.7999999999999999E-2]
["断熱材","チヨダウーテ株式会社","DTIYE21GW3","アースウール24K","D3","グラスウール断熱材高性能製品　HG24-36",3.5999999999999997E-2]
["断熱材","株式会社デコス","DDCS011CB3","デコスファイバー","D3","吹込み用セルロースファイバー２５Ｋ",0.04]
["断熱材","株式会社デコス","DDCS021CB3","デコスファイバー","D3","吹込み用セルロースファイバー５５Ｋ",0.04]
["断熱材","デュポン・スタイロ株式会社","DDOWX41XP1","スタイロフォームFG","D1","押出法ポリスチレンフォーム断熱材３種ｂD",2.1999999999999999E-2]
["断熱材","デュポン・スタイロ株式会社","DDOWX11XP2","スタイロエース-II","D2","押出法ポリスチレンフォーム断熱材３種ｂA",2.8000000000000001E-2]
["断熱材","デュポン・スタイロ株式会社","DDOWX21XP2","スタイロフォームAT","D2","押出法ポリスチレンフォーム断熱材３種ｂA",2.8000000000000001E-2]
["断熱材","デュポン・スタイロ株式会社","DDOWX31XP2","スタイロフォームEX","D2","押出法ポリスチレンフォーム断熱材３種ｂC",2.4E-2]
["断熱材","デュポン・スタイロ株式会社","DDOWX71XP2","スタイロフォームGK-II","D2","押出法ポリスチレンフォーム断熱材３種ｂAII",2.8000000000000001E-2]
["断熱材","デュポン・スタイロ株式会社","DDOWX81XP2","スタイロフォームRB-GK-II","D2","押出法ポリスチレンフォーム断熱材３種ｂAII",2.8000000000000001E-2]
["断熱材","デュポン・スタイロ株式会社","DDOWX51XP3","スタイロフォームIB","D3","押出法ポリスチレンフォーム断熱材１種ｂC",3.5999999999999997E-2]
["断熱材","デュポン・スタイロ株式会社","DDOWX61XP3","スタイロフォームTM","D3","押出法ポリスチレンフォーム断熱材２種ｂA",3.4000000000000002E-2]
["断熱材","東北資材工業株式会社","DE06A11PE3","TSK16","D3","発泡プラスチック断熱材　ビーズ法ポリスチレンフォーム断熱材　4号",4.1000000000000002E-2]
["断熱材","東北資材工業株式会社","DE06A21PE3","TSK20","D3","発泡プラスチック断熱材　ビーズ法ポリスチレンフォーム断熱材　3号",3.7999999999999999E-2]
["断熱材","東北資材工業株式会社","DE06A31PE3","TSK30","D3","発泡プラスチック断熱材　ビーズ法ポリスチレンフォーム断熱材　1号",3.4000000000000002E-2]
["断熱材","東北資材工業株式会社","DE06A41PE3","NB18","D3","発泡プラスチック断熱材　ビーズ法ポリスチレンフォーム断熱材　4号",4.1000000000000002E-2]
["断熱材","株式会社富岡産業","DT30T11TM3","スタイロ畳　富岡産業　建材畳床III型-50","D3","建材畳III型５０mm厚２５",4.1000000000000002E-2]
["断熱材","株式会社富岡産業","DT30T21TM3","スタイロ畳　富岡産業　建材畳床III型-55","D3","建材畳III型５５mm厚３０",0.04]
["断熱材","トーホー工業株式会社","DE48A11EP3","ﾄｰﾎｰﾌｫｰﾑ特号9511 1000×2000×500","D3","A種ビーズ法ポリスチレンフォーム保温板特号",3.4000000000000002E-2]
["断熱材","トーホー工業株式会社","DE48A21EP3","ﾄｰﾎｰﾌｫｰﾑ3号9511 1000×2000×500","D3","A種ビーズ法ポリスチレンフォーム保温板３号",0.04]
["断熱材","トーホー工業株式会社","DE48B11EP3","ﾄｰﾎｰﾌｫｰﾑ1号9521 1000×2000×500","D3","ビーズ法ポリスチレンフォーム断熱材１号",3.4000000000000002E-2]
["断熱材","トーホー工業株式会社","DE48B21EP3","ﾄｰﾎｰﾌｫｰﾑ3号9521 1000×2000×500","D3","ビーズ法ポリスチレンフォーム断熱材３号",3.7999999999999999E-2]
["断熱材","トーホー工業株式会社","DE48B31EP3","ﾄｰﾎｰﾌｫｰﾑ3号9521 910×605×100","D3","ビーズ法ポリスチレンフォーム断熱材３号",3.7999999999999999E-2]
["断熱材","トーホー工業株式会社","DE48B41EP3","ﾄｰﾎｰﾌｫｰﾑ4号9521 910×605×100","D3","ビーズ法ポリスチレンフォーム断熱材４号",4.1000000000000002E-2]
["断熱材","有限会社鍋屋商店","DTA1N11TM3","スタイロ畳　鍋屋商店　建材畳床II型-50","D3","建材畳II型５０mm厚３０",3.9E-2]
["断熱材","有限会社鍋屋商店","DTA1N21TM3","スタイロ畳　鍋屋商店　建材畳床II型-55","D3","建材畳II型５５mm厚３５",3.7999999999999999E-2]
["断熱材","有限会社鍋屋商店","DTA1N31TM3","スタイロ畳　鍋屋商店　建材畳床III型-50","D3","建材畳III型５０mm厚２５",4.1000000000000002E-2]
["断熱材","有限会社鍋屋商店","DTA1N41TM3","スタイロ畳　鍋屋商店　建材畳床III型-55","D3","建材畳II型５５mm厚３０",0.04]
["断熱材","有限会社鍋屋商店","DTA1N51TM3","スタイロ畳　鍋屋商店　建材畳床N型-50","D3","建材畳Ｎ型５０mm厚４５",3.4000000000000002E-2]
["断熱材","有限会社鍋屋商店","DTA1N61TM3","スタイロ畳　鍋屋商店　建材畳床N型-55","D3","建材畳Ｎ型５５mm厚５０",3.4000000000000002E-2]
["断熱材","ニチアス株式会社","DNCAA61RW3","MGビルパックF","D3","ロックウール断熱材MB",3.6999999999999998E-2]
["断熱材","ニチアス株式会社","DNCAA71RW3","ホームマットF","D3","ロックウール断熱材MB",3.6999999999999998E-2]
["断熱材","ニチアス株式会社","DNCA011RW3","ホームマット","D3","ロックウール断熱材（マット）",3.7999999999999999E-2]
["断熱材","ニチアス株式会社","DNCA021RW3","ホームマットNEO","D3","ロックウール断熱材（マット）",3.7999999999999999E-2]
["断熱材","ニチアス株式会社","DNCAA31RW3","ホームマット F","D3","ロックウール断熱材（マット）",3.7999999999999999E-2]
["断熱材","ニチアス株式会社","DNCAA41RW3","MGビルパック","D3","ロックウール断熱材（マット）",3.7999999999999999E-2]
["断熱材","ニチアス株式会社","DNCAA51RW3","MGビルパック　F","D3","ロックウール断熱材（マット）",3.7999999999999999E-2]
["断熱材","日清紡ケミカル株式会社","DNISC43PS2","SG-900","D2","吹付硬質ウレタンフォームA種1H",2.5999999999999999E-2]
["断熱材","日清紡ケミカル株式会社","DNIS013PS3","SF-100","D3","吹付け硬質ウレタンフォームA種３",0.04]
["断熱材","日清紡ケミカル株式会社","DNIS023PS3","SI-NFS","D3","吹付け硬質ウレタンフォームA種１",3.3000000000000002E-2]
["断熱材","日清紡ケミカル株式会社","DNISC33PS3","SF-120","D3","吹付硬質ウレタンフォームA種３",0.04]
["断熱材","日本製紙木材株式会社","DNPL011CB3","スーパージェットファイバー","D3","吹込み用セルロースファイバー２５Ｋ",0.04]
["断熱材","日本製紙木材株式会社","DNPL021CB3","スーパージェットファイバー","D3","吹込み用セルロースファイバー５０Ｋ",0.04]
["断熱材","株式会社日本アクア","DS20A13PS2","アクアフォームNEO","D2","吹付け硬質ウレタンフォームA種１H",2.5999999999999999E-2]
["断熱材","株式会社日本アクア","DS20013PS3","アクアフォーム-R","D3","吹付け硬質ウレタンフォームA種３",3.5999999999999997E-2]
["断熱材","株式会社日本アクア","DS20A23PS3","アクアAフォーム","D3","吹付け硬質ウレタンフォームA種１",3.4000000000000002E-2]
["断熱材","株式会社日本アクア","DS20A33PS3","アクアフォーム","D3","吹付け硬質ウレタンフォームA種３",0.04]
["断熱材","日本パフテム株式会社","DNPCA13PS2","パフピュアーエース","D2","吹付け硬質ウレタンフォームA種１H",2.5999999999999999E-2]
["断熱材","日本パフテム株式会社","DNPC013PS3","MOCOフォーム","D3","吹付け硬質ウレタンフォームA種３",0.04]
["断熱材","日本ロックウール株式会社","DNRWW21RB3","ホームブローウール(屋根・床・壁用)","D3","吹込み用ロックウール６５Ｋ相当",3.7999999999999999E-2]
["断熱材","日本ロックウール株式会社","DNRWC24RB4","ホームブローウール(天井用)","D4","天井断熱工事用吹込みロックウール２５Ｋ",4.7E-2]
["断熱材","株式会社浜中たたみ店","DT19011TM3","和やか畳床","D3","建材畳III型５０mm厚２５",4.1000000000000002E-2]
["断熱材","パラマウント硝子工業株式会社","DPGMC41GW2","太陽SUNR(SRG)","D2","グラスウール断熱材 高性能品GWHG38-32",3.2000000000000001E-2]
["断熱材","パラマウント硝子工業株式会社","DPGM041GW3","太陽SUN","D3","グラスウール断熱材 高性能品GWHG16-38",3.7999999999999999E-2]
["断熱材","パラマウント硝子工業株式会社","DPGM051GW3","太陽SUN","D3","グラスウール断熱材 高性能品GWHG24-36",3.5999999999999997E-2]
["断熱材","パラマウント硝子工業株式会社","DPGM052GB3","サンブロードライ(BIBZ2R)","D3","吹込み用グラスウール断熱材　LFGW3238",3.7999999999999999E-2]
["断熱材","パラマウント硝子工業株式会社","DPGM071GW3","太陽SUNボード外断","D3","グラスウール断熱材 高性能品GWHG32-35",3.5000000000000003E-2]
["断熱材","パラマウント硝子工業株式会社","DPGM081GW3","太陽SUNﾎﾞｰﾄﾞ","D3","グラスウール断熱材 高性能品GWHG32-35",3.5000000000000003E-2]
["断熱材","パラマウント硝子工業株式会社","DPGM101GW3","ハウスロンプレミア","D3","グラスウール断熱材 高性能品GWHG16-38",3.7999999999999999E-2]
["断熱材","パラマウント硝子工業株式会社","DPGM111GW3","露断プレミア","D3","グラスウール断熱材 GW32-36",3.5999999999999997E-2]
["断熱材","パラマウント硝子工業株式会社","DPGM131GW3","FGHG","D3","グラスウール断熱材 高性能品GWHG16-38",3.7999999999999999E-2]
["断熱材","パラマウント硝子工業株式会社","DPGM141GW3","HGS","D3","グラスウール断熱材 高性能品GWHG16-38",3.7999999999999999E-2]
["断熱材","パラマウント硝子工業株式会社","DPGM151GW3","FGHG","D3","グラスウール断熱材 高性能品GWHG24-36",3.5999999999999997E-2]
["断熱材","パラマウント硝子工業株式会社","DPGMA11GW3","太陽SUNR","D3","グラスウール断熱材 高性能品GWHG20-35",3.5000000000000003E-2]
["断熱材","パラマウント硝子工業株式会社","DPGMA21GW3","内装パラダイス","D3","グラスウール断熱材 GW24-38",3.7999999999999999E-2]
["断熱材","パラマウント硝子工業株式会社","DPGMC11GW3","露断ピンレス","D3","グラスウール断熱材 GW32-36",3.5999999999999997E-2]
["断熱材","パラマウント硝子工業株式会社","DPGMC21GW3","ハウスロンZERO","D3","グラスウール断熱材 高性能品GWHG16-38",3.7999999999999999E-2]
["断熱材","パラマウント硝子工業株式会社","DPGMC24GB3","サンブロードライ(BIBZ2RR)","D3","吹込み用グラスウール断熱材　LFGW4036",3.5999999999999997E-2]
["断熱材","パラマウント硝子工業株式会社","DPGMC31GW3","ハウスロンZERO(HZD)","D3","グラスウール断熱材 高性能品GWHG24-35",3.5000000000000003E-2]
["断熱材","パラマウント硝子工業株式会社","DPGM014GB4","ニューダンブロー","D4","吹込み用グラスウール断熱材　天井用　　LFGW1852",5.1999999999999998E-2]
["断熱材","パラマウント硝子工業株式会社","DPGM084GB4","サンブロードライ(BIBZ1R)","D4","吹込み用グラスウール断熱材　天井用　　LFGW1352",5.1999999999999998E-2]
["断熱材","BASF INOAC ポリウレタン株式会社","DBIPS23PS2","フォームライト・エコ　EB","D2","吹付け硬質ウレタンフォームA種1H",2.5999999999999999E-2]
["断熱材","BASF INOAC ポリウレタン株式会社","DBIPS33PS2","フォームライト　SL-50α","D2","建築物断熱用吹付け硬質ウレタンフォーム　A種１H",2.5999999999999999E-2]
["断熱材","BASF INOAC ポリウレタン株式会社","DBIP013PS3","フォームライトSL","D3","吹付け硬質ウレタンフォームA種３",0.04]
["断熱材","BASF INOAC ポリウレタン株式会社","DBIPS13PS3","フォームライト・エコ　LC","D3","吹付け硬質ウレタンフォームA種１",3.4000000000000002E-2]
["断熱材","BASF INOAC ポリウレタン株式会社","DBIPS43PS3","フォームライト　SL-100AT","D3","建築物断熱用吹付け硬質ウレタンフォーム　A種３",0.04]
["断熱材","フクビ化学工業株式会社","DFVKJ11PH1","フェノバボード","D1","フェノールフォーム保温板１種２号D",1.9E-2]
["断熱材","フクビ化学工業株式会社","DFVKL12PH1","フェノバボードJ","D1","フェノールフォーム保温板3種1号A",1.9E-2]
["断熱材","フクビ化学工業株式会社","DFVKV11PH1","フェノバボード遮熱","D1","フェノールフォーム保温板１種２号D",1.9E-2]
["断熱材","フクビ化学工業株式会社","DFVK015MI3","フクフォームEco　E-3335型","D3","その他",0.04]
["断熱材","フクビ化学工業株式会社","DFVK025MI3","フクフォームEco　E-33J89型","D3","その他",0.04]
["断熱材","フクビ化学工業株式会社","DFVK035MI3","フクフォームEco　E-33J98型","D3","その他",3.5999999999999997E-2]
["断熱材","フクビ化学工業株式会社","DFVKA15MI3","フクフォームEco","D3","その他",3.5999999999999997E-2]
["断熱材","マグ・イゾベール株式会社","DMAG051GW3","床トップ","D3","グラスウール断熱材　通常品　GW32-36",3.5999999999999997E-2]
["断熱材","マグ・イゾベール株式会社","DMAG061GW3","床トップ剛床","D3","グラスウール断熱材　通常品　GW32-36",3.5999999999999997E-2]
["断熱材","マグ・イゾベール株式会社","DMAG071GW3","マグロール","D3","グラスウール断熱材　通常品　GW24-38",3.7999999999999999E-2]
["断熱材","マグ・イゾベール株式会社","DMAG081GW3","住宅用グラスウールA","D3","グラスウール断熱材　通常品　GW24-38",3.7999999999999999E-2]
["断熱材","マグ・イゾベール株式会社","DMAG091GW3","住宅用グラスウールA","D3","グラスウール断熱材　通常品　GW32-36",3.5999999999999997E-2]
["断熱材","マグ・イゾベール株式会社","DMAG111GW3","住宅用グラスウールA","D3","グラスウール断熱材　高性能品　GWHG16-38",3.7999999999999999E-2]
["断熱材","マグ・イゾベール株式会社","DMAG121GW3","住宅用グラスウールA","D3","グラスウール断熱材　高性能品　GWHG20-36",3.5999999999999997E-2]
["断熱材","マグ・イゾベール株式会社","DMAG131GW3","住宅用グラスウールA","D3","グラスウール断熱材　高性能品　GWHG24-36",3.5999999999999997E-2]
["断熱材","マグ・イゾベール株式会社","DMAG141GW3","住宅用グラスウールB","D3","グラスウール断熱材　高性能品　GWHG16-38",3.7999999999999999E-2]
["断熱材","マグ・イゾベール株式会社","DMAG151GW3","住宅用グラスウールB","D3","グラスウール断熱材　高性能品　GWHG24-36",3.5999999999999997E-2]
["断熱材","マグ・イゾベール株式会社","DMAG161GW3","住宅用グラスウールC","D3","グラスウール断熱材　高性能品　GWHG16-38",3.7999999999999999E-2]
["断熱材","マグ・イゾベール株式会社","DMAG171GW3","住宅用グラスウールC","D3","グラスウール断熱材　高性能品　GWHG24-36",3.5999999999999997E-2]
["断熱材","マグ・イゾベール株式会社","DMAG181GW3","住宅用グラスウールC","D3","グラスウール断熱材　通常品　GW24-38",3.7999999999999999E-2]
["断熱材","マグ・イゾベール株式会社","DMAG191GW3","住宅用グラスウールC","D3","グラスウール断熱材　通常品　GW32-36",3.5999999999999997E-2]
["断熱材","マグ・イゾベール株式会社","DMAG201GW3","住宅用グラスウールD","D3","グラスウール断熱材　高性能品　GWHG16-38",3.7999999999999999E-2]
["断熱材","マグ・イゾベール株式会社","DMAG211GW3","住宅用グラスウールD","D3","グラスウール断熱材　高性能品　GWHG24-36",3.5999999999999997E-2]
["断熱材","マグ・イゾベール株式会社","DMAG221GW3","住宅用グラスウールD","D3","グラスウール断熱材　通常品　GW24-38",3.7999999999999999E-2]
["断熱材","マグ・イゾベール株式会社","DMAG231GW3","住宅用グラスウールD","D3","グラスウール断熱材　通常品　GW32-36",3.5999999999999997E-2]
["断熱材","マグ・イゾベール株式会社","DMAG241GW3","住宅用グラスウールE","D3","グラスウール断熱材　高性能品　GWHG16-38",3.7999999999999999E-2]
["断熱材","マグ・イゾベール株式会社","DMAG251GW3","住宅用グラスウールE","D3","グラスウール断熱材　通常品　GW24-38",3.7999999999999999E-2]
["断熱材","マグ・イゾベール株式会社","DMAG261GW3","住宅用グラスウールE","D3","グラスウール断熱材　通常品　GW32-36",3.5999999999999997E-2]
["断熱材","マグ・イゾベール株式会社","DMAG271GW3","住宅用グラスウールE","D3","グラスウール断熱材　通常品　GW32-36",3.5999999999999997E-2]
["断熱材","マグ・イゾベール株式会社","DMAGA11GW3","住宅用グラスウールA","D3","グラスウール断熱材　保温板　40K",3.5999999999999997E-2]
["断熱材","マグ・イゾベール株式会社","DMAGB21GW3","床リノベ","D3","グラスウール断熱材　高性能品　GWHG16-38",3.7999999999999999E-2]
["断熱材","マグ・イゾベール株式会社","DMAGB31GW3","床リノベ","D3","グラスウール断熱材　通常品　GW32-36",3.5999999999999997E-2]
["断熱材","マグ・イゾベール株式会社","DMAGC11GW3","イゾベール・コンフォート","D3","グラスウール断熱材　高性能品　GWHG16-38",3.7999999999999999E-2]
["断熱材","マグ・イゾベール株式会社","DMAGC21GW3","イゾベール・コンフォート","D3","グラスウール断熱材　高性能品　GWHG24-35",3.5000000000000003E-2]
["断熱材","マグ・イゾベール株式会社","DMAGC24GB3","マグブローライト","D3","吹込み用グラスウール断熱材　屋根・床・壁　LFGW2238",3.7999999999999999E-2]
["断熱材","マグ・イゾベール株式会社","DMAGC31GW3","イゾベール・スタンダード","D3","グラスウール断熱材　高性能品　GWHG16-38",3.7999999999999999E-2]
["断熱材","マグ・イゾベール株式会社","DMAGC41GW3","イゾベール・スタンダード","D3","グラスウール断熱材　高性能品　GWHG24-35",3.5000000000000003E-2]
["断熱材","マグ・イゾベール株式会社","DMAGC51GW3","付加断ボード","D3","グラスウール断熱材　高性能品　GWHG32-35",3.5000000000000003E-2]
["断熱材","マグ・イゾベール株式会社","DMAGC61GW3","床トップ120","D3","グラスウール断熱材　通常品　GW32-36",3.5999999999999997E-2]
["断熱材","マグ・イゾベール株式会社","DMAGC81GW3","イゾベール・コンフォート","D3","グラスウール断熱材　高性能品　GWHG28-33",3.3000000000000002E-2]
["断熱材","マグ・イゾベール株式会社","DMAGC91GW3","高性能グラスウールFV","D3","グラスウール断熱材　高性能品　GWHG16-38",3.7999999999999999E-2]
["断熱材","マグ・イゾベール株式会社","DMAGD11GW3","住宅用グラスウールD","D3","グラスウール断熱材　高性能品　GWHG24-35",3.5000000000000003E-2]
["断熱材","マグ・イゾベール株式会社","DMAG014GB4","マグブロー","D4","吹込み用グラスウール断熱材　天井用　LFGW1852",5.1999999999999998E-2]
["断熱材","マグ・イゾベール株式会社","DMAGC14GB4","マグブローライト","D4","吹込み用グラスウール断熱材　天井用　LFGW1052",5.1999999999999998E-2]
["断熱材","株式会社マツナガ","DMAT011CB3","MSグリーンファイバー","D3","吹込み用セルロースファイバー６０Ｋ",0.04]
["断熱材","松原産業株式会社","DMBSP13EP3","パイナルフォーム1号","D3","A種ビーズ法ポリスチレンフォーム保温板１号",3.4000000000000002E-2]
["断熱材","松原産業株式会社","DMBSP33EP3","パイナルフォーム3号","D3","A種ビーズ法ポリスチレンフォーム保温板３号",3.5999999999999997E-2]
["断熱材","松原産業株式会社","DMBSP43EP3","パイナルフォーム4号","D3","A種ビーズ法ポリスチレンフォーム保温板４号",3.9E-2]
["断熱材","株式会社丸清","DT18011TM3","スタイロ畳　丸清　建材畳床-50","D3","建材畳III型５０mm厚２５",4.1000000000000002E-2]
["断熱材","株式会社丸清","DT18021TM3","スタイロ畳　丸清　建材畳床-55","D3","建材畳III型５５mm厚３０",0.04]
["断熱材","三井化学アグロ株式会社","DMKAA13PS3","ヒートマジックシステム (アクトコールSK-1736、コスモネートM-200)","D3","建築物断熱用吹付け硬質ウレタンフォームA種3",3.7999999999999999E-2]
["断熱材","三ツ星ベルト株式会社","DMITH11PU2","ネオハードフォーム25","D2","硬質ウレタンフォーム断熱材PUF3.1D",2.3E-2]
["断熱材","三ツ星ベルト株式会社","DMITH21PU2","ネオハードフォーム30","D2","硬質ウレタンフォーム断熱材PUF3.1D",2.3E-2]
["断熱材","三ツ星ベルト株式会社","DMITH31PU2","ネオハードフォーム35","D2","硬質ウレタンフォーム断熱材PUF3.1D",2.3E-2]
["断熱材","三ツ星ベルト株式会社","DMITH41PU2","ネオハードフォーム40","D2","硬質ウレタンフォーム断熱材PUF3.1D",2.3E-2]
["断熱材","三ツ星ベルト株式会社","DMITH51PU2","ネオハードフォーム50","D2","硬質ウレタンフォーム断熱材PUF3.1D",2.3E-2]
["断熱材","吉水商事株式会社","DYOS011CB3","ファイバーエース","D3","吹込み用セルロースファイバー２５Ｋ",0.04]
["断熱材","吉水商事株式会社","DYOS021CB3","ファイバーエース","D3","吹込み用セルロースファイバー５５Ｋ",0.04]
["断熱材","株式会社LIXIL","DS82A33PU1","ウレタン断熱パネル","D1","硬質ウレタンフォーム断熱材1種2号相当品",1.9E-2]
["断熱材","株式会社LIXIL","DS82015VP1","ウォール インプラス","D1","真空断熱材",3.0000000000000001E-3]
["断熱材","株式会社LIXIL","DS82025VP1","フロア インプラス","D1","真空断熱材",3.0000000000000001E-3]
["断熱材","株式会社ワンワールド","DOWTA11GW3","山びこHGS","D3","グラスウール断熱材　通常品　24-38",3.7999999999999999E-2]
["断熱材","株式会社ワンワールド","DOWTA21GW3","テクノEセーブ H16K","D3","グラスウール断熱材　高性能品　HG16-38",3.7999999999999999E-2]
["断熱材","株式会社ワンワールド","DOWTA31GW3","テクノEセーブ H24K","D3","グラスウール断熱材　高性能品　HG24-36",3.5999999999999997E-2]
["断熱材","株式会社ワンワールド","DOWTA41GW3","テクノマックスJ","D3","グラスウール断熱材　高性能品　HG16-38",3.7999999999999999E-2]
["断熱材","株式会社ワンワールド","DOWTB11GW3","グラスウール断熱材 NA","D3","グラスウール断熱材　通常品　24-38",3.7999999999999999E-2]
["断熱材","株式会社ワンワールド","DOWTB21GW3","グラスウール断熱材 NB","D3","グラスウール断熱材　通常品　32-36",3.5999999999999997E-2]
["断熱材","株式会社ワンワールド","DOWTB31GW3","グラスウール断熱材 NC","D3","グラスウール断熱材　通常品　40-36",3.5999999999999997E-2]
["断熱材","株式会社ワンワールド","DOWTB41GW3","高性能グラスウール断熱材 HA","D3","グラスウール断熱材　高性能品　HG16-38",3.7999999999999999E-2]
["断熱材","株式会社ワンワールド","DOWTB51GW3","高性能グラスウール断熱材 HB","D3","グラスウール断熱材　高性能品　HG24-36",3.5999999999999997E-2]
["断熱材","株式会社ワンワールド","DOWTB61GW3","高性能グラスウール断熱材 HC","D3","グラスウール断熱材　高性能品　HG32-35",3.5000000000000003E-2]
["断熱材","株式会社ワンワールド","DOWTB71GW3","高性能グラスウール断熱材 HD","D3","グラスウール断熱材　高性能品　HG40-34",3.4000000000000002E-2]
["断熱材","株式会社ワンワールド","DOWT014GB4","テクノブロー","D4","天井断熱工事用吹込みグラスウール１８Ｋ",5.1999999999999998E-2]
["ガラス","IGウインドウズ株式会社","GIC052N1","アルゴンガス入り遮熱Low-E複層ガラス(SLGY)グリーン","G1",null,null,"アルゴンガス",11,null,"無"]
["ガラス","IGウインドウズ株式会社","GIC062Y1","AT付アルゴンガス入り遮熱Low-E複層ガラス(SLGB)ブルー","G1",null,null,"アルゴンガス",10,null,"有"]
["ガラス","IGウインドウズ株式会社","GIC072N1","アルゴンガス入り遮熱Low-E複層ガラス(SLGB)ブルー","G1",null,null,"アルゴンガス",10,null,"無"]
["ガラス","IGウインドウズ株式会社","GIC092N1","アルゴンガス入り遮熱Low-E防犯複層ガラス(SLGY)グリーン","G1",null,null,"アルゴンガス",11,null,"無"]
["ガラス","IGウインドウズ株式会社","GIC112N1","アルゴンガス入り遮熱Low-E防犯複層ガラス(SLGB)ブルー","G1",null,null,"アルゴンガス",10,null,"無"]
["ガラス","IGウインドウズ株式会社","GICA11N1","遮熱Low-E複層ガラス(SLGY)グリーン","G1",null,null,"乾燥空気",15,null,"無"]
["ガラス","IGウインドウズ株式会社","GICA41N1","遮熱Low-E複層ガラス(SLGB)ブルー","G1",null,null,"乾燥空気",15,null,"無"]
["ガラス","IGウインドウズ株式会社","GICA51N1","遮熱Low-E防犯複層ガラス(SLGY)グリーン","G1",null,null,"乾燥空気",15,null,"無"]
["ガラス","IGウインドウズ株式会社","GICA81N1","遮熱Low-E防犯複層ガラス(SLGB)ブルー","G1",null,null,"乾燥空気",15,null,"無"]
["ガラス","IGウインドウズ株式会社","GICC11N1","遮熱Low-E複層ガラス(SLGJ)グリーン","G1",null,null,"乾燥空気",15,null,"無"]
["ガラス","IGウインドウズ株式会社","GICC12N1","アルゴンガス入り遮熱Low-E複層ガラス(SLGJ)グリーン","G1",null,null,"アルゴンガス",11,null,"無"]
["ガラス","IGウインドウズ株式会社","GICC21N1","断熱Low-E複層ガラス(DLGP)クリア","G1",null,null,"乾燥空気",15,null,"無"]
["ガラス","IGウインドウズ株式会社","GICC22N1","アルゴンガス入り断熱Low-E複層ガラス(DLGP)クリア","G1",null,null,"アルゴンガス",11,null,"無"]
["ガラス","IGウインドウズ株式会社","GIC032Y2","AT付アルゴンガス入り遮熱Low-E複層ガラス(SLGY)グリーン","G2",null,null,"アルゴンガス",6,null,"有"]
["ガラス","IGウインドウズ株式会社","GIC041N2","断熱Low-E複層ガラス(DLGP)クリア","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","IGウインドウズ株式会社","GIC041Y2","AT付断熱Low-E複層ガラス(DLGP)クリア","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","IGウインドウズ株式会社","GIC042N2","アルゴンガス入り遮熱Low-E複層ガラス(SLGY)グリーン","G2",null,null,"アルゴンガス",6,null,"無"]
["ガラス","IGウインドウズ株式会社","GIC051N2","遮熱Low-E複層ガラス(SLGY)グリーン","G2",null,null,"乾燥空気",7,null,"無"]
["ガラス","IGウインドウズ株式会社","GIC051Y2","AT付遮熱Low-E複層ガラス(SLGY)グリーン","G2",null,null,"乾燥空気",7,null,"有"]
["ガラス","IGウインドウズ株式会社","GIC052Y2","AT付アルゴンガス入り遮熱Low-E複層ガラス(SLGB)ブルー","G2",null,null,"アルゴンガス",6,null,"有"]
["ガラス","IGウインドウズ株式会社","GIC062N2","アルゴンガス入り遮熱Low-E複層ガラス(SLGB)ブルー","G2",null,null,"アルゴンガス",6,null,"無"]
["ガラス","IGウインドウズ株式会社","GIC071N2","遮熱Low-E複層ガラス(SLGB)ブルー","G2",null,null,"乾燥空気",7,null,"無"]
["ガラス","IGウインドウズ株式会社","GIC071Y2","AT付遮熱Low-E複層ガラス(SLGB)ブルー","G2",null,null,"乾燥空気",7,null,"有"]
["ガラス","IGウインドウズ株式会社","GIC081N2","遮熱Low-E防犯複層ガラス(SLGY)グリーン","G2",null,null,"乾燥空気",7,null,"無"]
["ガラス","IGウインドウズ株式会社","GIC082N2","アルゴンガス入り遮熱Low-E防犯複層ガラス(SLGY)グリーン","G2",null,null,"アルゴンガス",6,null,"無"]
["ガラス","IGウインドウズ株式会社","GIC101N2","遮熱Low-E防犯複層ガラス(SLGB)ブルー","G2",null,null,"乾燥空気",7,null,"無"]
["ガラス","IGウインドウズ株式会社","GIC102N2","アルゴンガス入り遮熱Low-E防犯複層ガラス(SLGB)ブルー","G2",null,null,"アルゴンガス",6,null,"無"]
["ガラス","IGウインドウズ株式会社","GICC11N2","遮熱Low-E複層ガラス(SLGJ)グリーン","G2",null,null,"乾燥空気",7,null,"無"]
["ガラス","IGウインドウズ株式会社","GICC11Y2","At付遮熱Low-E複層ガラス(SLGJ)グリーン","G2",null,null,"乾燥空気",7,null,"有"]
["ガラス","IGウインドウズ株式会社","GICC12N2","アルゴンガス入り遮熱Low-E複層ガラス(SLGJ)グリーン","G2",null,null,"アルゴンガス",8,null,"無"]
["ガラス","IGウインドウズ株式会社","GICC12Y2","AT付アルゴンガス入り遮熱Low-E複層ガラス(SLGJ)グリーン","G2",null,null,"アルゴンガス",8,null,"有"]
["ガラス","IGウインドウズ株式会社","GICC22N2","アルゴンガス入り断熱Low-E複層ガラス(DLGP)クリア","G2",null,null,"アルゴンガス",8,null,"無"]
["ガラス","IGウインドウズ株式会社","GICC22Y2","AT付アルゴンガス入り断熱Low-E複層ガラス(DLGP)クリア","G2",null,null,"アルゴンガス",8,null,"有"]
["ガラス","AGC株式会社","GAG011N1","サンバランス　アクアグリーン","G1",null,null,"乾燥空気",14,null,"無"]
["ガラス","AGC株式会社","GAG012N1","サンバランス　アクアグリーン","G1",null,null,"アルゴンガス",10,null,"無"]
["ガラス","AGC株式会社","GAG012Y1","ペヤプラス　アクアグリーン","G1",null,null,"アルゴンガス",10,null,"有"]
["ガラス","AGC株式会社","GAG031N1","サンバランス　ピュアクリア","G1",null,null,"乾燥空気",15,null,"無"]
["ガラス","AGC株式会社","GAG032N1","サンバランス　ピュアクリア","G1",null,null,"アルゴンガス",11,null,"無"]
["ガラス","AGC株式会社","GAG032Y1","ペヤプラス　ピュアクリア","G1",null,null,"アルゴンガス",11,null,"有"]
["ガラス","AGC株式会社","GAG052N1","サンバランス　シルバー","G1",null,null,"アルゴンガス",13,null,"無"]
["ガラス","AGC株式会社","GAG052Y1","ペヤプラス　シルバー","G1",null,null,"アルゴンガス",13,null,"有"]
["ガラス","AGC株式会社","GAG071N1","サンバランス　プレミアムクール","G1",null,null,"乾燥空気",14,null,"無"]
["ガラス","AGC株式会社","GAG072N1","サンバランス　プレミアムクール","G1",null,null,"アルゴンガス",10,null,"無"]
["ガラス","AGC株式会社","GAG072Y1","ペヤプラス　プレミアムクール","G1",null,null,"アルゴンガス",10,null,"有"]
["ガラス","AGC株式会社","GAG131N1","サンバランス　サファイアブルー","G1",null,null,"乾燥空気",14,null,"無"]
["ガラス","AGC株式会社","GAG132N1","サンバランス　サファイアブルー","G1",null,null,"アルゴンガス",10,null,"無"]
["ガラス","AGC株式会社","GAG132Y1","ペヤプラス　サファイアブルー","G1",null,null,"アルゴンガス",10,null,"有"]
["ガラス","AGC株式会社","GAG011Y2","ペヤプラス・エア　アクアグリーン","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","AGC株式会社","GAG021N2","サンバランス　アクアグリーン","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","AGC株式会社","GAG021Y2","ペヤプラス・エア　ピュアクリア","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","AGC株式会社","GAG022N2","サンバランス　アクアグリーン","G2",null,null,"アルゴンガス",5,null,"無"]
["ガラス","AGC株式会社","GAG022Y2","ペヤプラス　アクアグリーン","G2",null,null,"アルゴンガス",5,null,"有"]
["ガラス","AGC株式会社","GAG031Y2","ペヤプラス・エア　シルバー","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","AGC株式会社","GAG041N2","サンバランス　ピュアクリア","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","AGC株式会社","GAG041Y2","ペヤプラス・エア　プレミアムクール","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","AGC株式会社","GAG042N2","サンバランス　ピュアクリア","G2",null,null,"アルゴンガス",5,null,"無"]
["ガラス","AGC株式会社","GAG042Y2","ペヤプラス　ピュアクリア","G2",null,null,"アルゴンガス",5,null,"有"]
["ガラス","AGC株式会社","GAG061N2","サンバランス　シルバー","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","AGC株式会社","GAG062N2","サンバランス　シルバー","G2",null,null,"アルゴンガス",6,null,"無"]
["ガラス","AGC株式会社","GAG062Y2","ペヤプラス　シルバー","G2",null,null,"アルゴンガス",6,null,"有"]
["ガラス","AGC株式会社","GAG071Y2","ペヤプラス・エア　サファイアブルー","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","AGC株式会社","GAG081N2","サンバランス　プレミアムクール","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","AGC株式会社","GAG082N2","サンバランス　プレミアムクール","G2",null,null,"アルゴンガス",5,null,"無"]
["ガラス","AGC株式会社","GAG082Y2","ペヤプラス　プレミアムクール","G2",null,null,"アルゴンガス",5,null,"有"]
["ガラス","AGC株式会社","GAG141N2","サンバランス　サファイアブルー","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","AGC株式会社","GAG142N2","サンバランス　サファイアブルー","G2",null,null,"アルゴンガス",5,null,"無"]
["ガラス","AGC株式会社","GAG142Y2","ペヤプラス　サファイアブルー","G2",null,null,"アルゴンガス",5,null,"有"]
["ガラス","AGC株式会社","GAGS13N2","ペアスマート","G2",null,null,"クリプトンガス",4,null,"無"]
["ガラス","株式会社栗原","GKG021N1","アイジーペア遮熱","G1",null,null,"乾燥空気",14,null,"無"]
["ガラス","株式会社栗原","GKG041N1","アイジーペア断熱","G1",null,null,"乾燥空気",15,null,"無"]
["ガラス","株式会社栗原","GKG011N2","アイジーペア遮熱","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","株式会社栗原","GKG031N2","アイジーペア断熱","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","株式会社サンシバ複層","GBFC11Y2","ホームエミネントペアLOW-E","G2",null,null,"乾燥空気",9,null,"有"]
["ガラス","セントラル硝子株式会社","GCG222N1","ペアレックスツインガードG　グリーン","G1",null,null,"アルゴンガス",11,null,"無"]
["ガラス","セントラル硝子株式会社","GCGB32N1","ペアレックスツインガードG　ブルー","G1",null,null,"アルゴンガス",10,null,"無"]
["ガラス","セントラル硝子株式会社","GCGC32N1","ペアレックスヒートガードG　グリーン","G1",null,null,"アルゴンガス",10,null,"無"]
["ガラス","セントラル硝子株式会社","GCGC52N1","ペアレックスヒートガードG　ブルー","G1",null,null,"アルゴンガス",10,null,"無"]
["ガラス","セントラル硝子株式会社","GCGD12N1","ペアレックスツインガードG　クリア","G1",null,null,"アルゴンガス",14,null,"無"]
["ガラス","セントラル硝子株式会社","GCGD22N1","ペアレックスツインガードG　シルバー","G1",null,null,"アルゴンガス",14,null,"無"]
["ガラス","セントラル硝子株式会社","GCGD32N1","ペアレックスヒートガードG　クリア","G1",null,null,"アルゴンガス",14,null,"無"]
["ガラス","セントラル硝子株式会社","GCGD42N1","ペアレックスヒートガードG　シルバー","G1",null,null,"アルゴンガス",14,null,"無"]
["ガラス","セントラル硝子株式会社","GCGD51N1","ペアレックスツインガード　グリーン","G1",null,null,"乾燥空気",14,null,"無"]
["ガラス","セントラル硝子株式会社","GCGD61N1","ペアレックスツインガード　ブルー","G1",null,null,"乾燥空気",14,null,"無"]
["ガラス","セントラル硝子株式会社","GCGD71N1","ペアレックスヒートガード　グリーン","G1",null,null,"乾燥空気",14,null,"無"]
["ガラス","セントラル硝子株式会社","GCGD81N1","ペアレックスヒートガード　ブルー","G1",null,null,"乾燥空気",14,null,"無"]
["ガラス","セントラル硝子株式会社","GCG011N2","ペアレックスツインガード　シルバー","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","セントラル硝子株式会社","GCG021N2","ペアレックスツインガード　グリーン","G2",null,null,"乾燥空気",7,null,"無"]
["ガラス","セントラル硝子株式会社","GCG031N2","ペアレックスツインガード　クリア","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","セントラル硝子株式会社","GCG041N2","ペアレックスツインガード　ブルー","G2",null,null,"乾燥空気",7,null,"無"]
["ガラス","セントラル硝子株式会社","GCG051N2","ペアレックスヒートガード　シルバー","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","セントラル硝子株式会社","GCG111Y2","ホームペアレックスS　ツインガード　シルバー","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","セントラル硝子株式会社","GCG121Y2","ホームペアレックスS　ツインガード　グリーン","G2",null,null,"乾燥空気",7,null,"有"]
["ガラス","セントラル硝子株式会社","GCG131Y2","ホームペアレックスS　ツインガード　クリア","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","セントラル硝子株式会社","GCG141Y2","ホームペアレックスS　ツインガード　ブルー","G2",null,null,"乾燥空気",7,null,"有"]
["ガラス","セントラル硝子株式会社","GCG151Y2","ホームペアレックスS　ヒートガード　シルバー","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","セントラル硝子株式会社","GCG212N2","ペアレックスツインガードG　シルバー","G2",null,null,"アルゴンガス",6,null,"無"]
["ガラス","セントラル硝子株式会社","GCG232N2","ペアレックスツインガードG　グリーン","G2",null,null,"アルゴンガス",5,null,"無"]
["ガラス","セントラル硝子株式会社","GCG242N2","ペアレックスヒートガードG　シルバー","G2",null,null,"アルゴンガス",6,null,"無"]
["ガラス","セントラル硝子株式会社","GCG312Y2","ホームペアレックスS　ツインガードG　シルバー","G2",null,null,"アルゴンガス",6,null,"有"]
["ガラス","セントラル硝子株式会社","GCG322Y2","ホームペアレックスS　ツインガードG　グリーン","G2",null,null,"アルゴンガス",5,null,"有"]
["ガラス","セントラル硝子株式会社","GCG332Y2","ホームペアレックスS　ヒートガードG　シルバー","G2",null,null,"アルゴンガス",6,null,"有"]
["ガラス","セントラル硝子株式会社","GCGA11N2","ペアレックスヒートガード　クリア","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","セントラル硝子株式会社","GCGA11Y2","ホームペアレックスS　ヒートガード　クリア","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","セントラル硝子株式会社","GCGA21N2","ペアレックスヒートガード　グリーン","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","セントラル硝子株式会社","GCGA21Y2","ホームペアレックスS　ヒートガード　グリーン","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","セントラル硝子株式会社","GCGA31N2","ペアレックスヒートガード　ブルー","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","セントラル硝子株式会社","GCGA31Y2","ホームペアレックスS　ヒートガード　ブルー","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","セントラル硝子株式会社","GCGB12N2","ペアレックスツインガードG　クリア","G2",null,null,"アルゴンガス",6,null,"無"]
["ガラス","セントラル硝子株式会社","GCGB12Y2","ホームペアレックスS　ツインガードG　クリア","G2",null,null,"アルゴンガス",6,null,"有"]
["ガラス","セントラル硝子株式会社","GCGB22N2","ペアレックスツインガードG　ブルー","G2",null,null,"アルゴンガス",5,null,"無"]
["ガラス","セントラル硝子株式会社","GCGB22Y2","ホームペアレックスS　ツインガードG　ブルー","G2",null,null,"アルゴンガス",5,null,"有"]
["ガラス","セントラル硝子株式会社","GCGC12N2","ペアレックスヒートガードG　クリア","G2",null,null,"アルゴンガス",6,null,"無"]
["ガラス","セントラル硝子株式会社","GCGC12Y2","ホームペアレックスS　ヒートガードG　クリア","G2",null,null,"アルゴンガス",6,null,"有"]
["ガラス","セントラル硝子株式会社","GCGC22N2","ペアレックスヒートガードG　グリーン","G2",null,null,"アルゴンガス",5,null,"無"]
["ガラス","セントラル硝子株式会社","GCGC22Y2","ホームペアレックスS　ヒートガードG　グリーン","G2",null,null,"アルゴンガス",5,null,"有"]
["ガラス","セントラル硝子株式会社","GCGC42N2","ペアレックスヒートガードG　ブルー","G2",null,null,"アルゴンガス",5,null,"無"]
["ガラス","セントラル硝子株式会社","GCGC42Y2","ホームペアレックスS　ヒートガードG　ブルー","G2",null,null,"アルゴンガス",5,null,"有"]
["ガラス","日本板硝子株式会社","GNS014N1","スペーシア","G1",null,null,"真空",0.2,null,"無"]
["ガラス","日本板硝子株式会社","GNS024N1","スペーシアクール","G1",null,null,"真空",0.2,null,"無"]
["ガラス","日本板硝子株式会社","GNS114N1","スペーシア21","G1",null,null,"真空",9,0.2,"無"]
["ガラス","日本板硝子株式会社","GNS351N1","ペアマルチレイボーググリーン","G1",null,null,"乾燥空気",14,null,"無"]
["ガラス","日本板硝子株式会社","GNS361N1","ペアマルチレイボーグクリア","G1",null,null,"乾燥空気",14,null,"無"]
["ガラス","日本板硝子株式会社","GNS461N1","ペアマルチスーパーグリーン","G1",null,null,"乾燥空気",14,null,"無"]
["ガラス","日本板硝子株式会社","GNSN31N1","ペアマルチE4グリーン","G1",null,null,"乾燥空気",12,null,"無"]
["ガラス","日本板硝子株式会社","GNSN41N1","ペアマルチE4クリア","G1",null,null,"乾燥空気",12,null,"無"]
["ガラス","日本板硝子株式会社","GNSN81N1","ペアマルチスーパークリアS","G1",null,null,"乾燥空気",15,null,"無"]
["ガラス","日本板硝子株式会社","GNSN91N1","ペアマルチLow-EクリアK74","G1",null,null,"乾燥空気",15,null,"無"]
["ガラス","日本板硝子株式会社","GNSV14N1","スーパースペーシア","G1",null,null,"真空",0.2,null,"無"]
["ガラス","日本板硝子株式会社","GNS211N2","ペアマルチEA","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","日本板硝子株式会社","GNS221N2","ペアマルチSE","G2",null,null,"乾燥空気",9,null,"無"]
["ガラス","日本板硝子株式会社","GNS311N2","ペアマルチレイボーググリーン","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","日本板硝子株式会社","GNS321N2","ペアマルチレイボーグクリア","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","日本板硝子株式会社","GNS421N2","ペアマルチスーパーグリーン","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","日本板硝子株式会社","GNSN11N2","ペアマルチE4グリーン","G2",null,null,"乾燥空気",5,null,"無"]
["ガラス","日本板硝子株式会社","GNSN21N2","ペアマルチE4クリア","G2",null,null,"乾燥空気",5,null,"無"]
["ガラス","日本板硝子株式会社","GNSN51Y2","ペアマルチレイボーググリーン","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","日本板硝子株式会社","GNSN81N2","ペアマルチスーパークリアS","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","日本板硝子株式会社","GNSN81Y2","ペアマルチスーパークリアS","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","日本板硝子株式会社","GNSN91N2","ペアマルチLow-EクリアK74","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","フィグラ株式会社","GFIF15N2","発熱ガラス　窓暖　　FL5+A12+EC5","G2",null,null,"その他",12,null,"無"]
["ガラス","フィグラ株式会社","GFIF25N2","発熱ガラス　窓暖　　Low-E5+A12+EC5","G2",null,null,"その他",12,null,"無"]
["ガラス","株式会社星野アルミ建材","GHA021N1","STELLA W S S","G1",null,null,"乾燥空気",16,null,"無"]
["ガラス","株式会社星野アルミ建材","GHA011N2","STELLA W S S","G2",null,null,"乾燥空気",12,null,"無"]
["ガラス","株式会社星野アルミ建材","GHA031N2","STELLA W S D","G2",null,null,"乾燥空気",12,null,"無"]
["ガラス","株式会社LIXIL","GLXA11N1","Low-E複層ガラスクリア(中空層15以上)","G1",null,null,"乾燥空気",15,null,"無"]
["ガラス","株式会社LIXIL","GLXA12N1","トリプルガラスクリアxクリアArガス入","G1",null,null,"アルゴンガス",6,6,"無"]
["ガラス","株式会社LIXIL","GLXA22N1","トリプルガラスグリーンxグリーンArガス入","G1",null,null,"アルゴンガス",6,6,"無"]
["ガラス","株式会社LIXIL","GLXA31N1","Low-E複層ガラスグリーン(中空層14以上)","G1",null,null,"乾燥空気",14,null,"無"]
["ガラス","株式会社LIXIL","GLXA32N1","トリプルガラスクリアxグリーンArガス入","G1",null,null,"アルゴンガス",6,6,"無"]
["ガラス","株式会社LIXIL","GLXA42N1","トリプルガラスクリアxブロンズArガス入","G1",null,null,"アルゴンガス",6,6,"無"]
["ガラス","株式会社LIXIL","GLXA51N1","Low-E複層ガラスグリーン高遮熱仕様(中空層14以上)","G1",null,null,"乾燥空気",14,null,"無"]
["ガラス","株式会社LIXIL","GLXA52N1","Low-E複層ガラスクリア(中空層Arガス入11以上)","G1",null,null,"アルゴンガス",11,null,"無"]
["ガラス","株式会社LIXIL","GLXA71N1","Low-E複層ガラスブロンズ(中空層15以上)","G1",null,null,"乾燥空気",15,null,"無"]
["ガラス","株式会社LIXIL","GLXA72N1","Low-E複層ガラスグリーン(中空層Arガス入10以上)","G1",null,null,"アルゴンガス",10,null,"無"]
["ガラス","株式会社LIXIL","GLXA92N1","Low-E複層ガラスグリーン高遮熱仕様(中空層Arガス入10以上)","G1",null,null,"アルゴンガス",10,null,"無"]
["ガラス","株式会社LIXIL","GLXB22N1","Low-E複層ガラスブロンズ(中空層Arガス入11以上)","G1",null,null,"アルゴンガス",11,null,"無"]
["ガラス","株式会社LIXIL","GLXB42Y1","AT付Low-E複層ガラスクリア(中空層Arガス入11～12)","G1",null,null,"アルゴンガス",11,null,"有"]
["ガラス","株式会社LIXIL","GLXB62Y1","AT付Low-E複層ガラスグリーン(中空層Arガス入10～12)","G1",null,null,"アルゴンガス",10,null,"有"]
["ガラス","株式会社LIXIL","GLXB82Y1","AT付Low-E複層ガラスグリーン高遮熱仕様(中空層Arガス入10～12)","G1",null,null,"アルゴンガス",10,null,"有"]
["ガラス","株式会社LIXIL","GLXC12Y1","AT付Low-E複層ガラスブロンズ(中空層Arガス入11～12)","G1",null,null,"アルゴンガス",11,null,"有"]
["ガラス","株式会社LIXIL","GLXC33N1","トリプルガラスクリアxクリアKrガス入り","G1",null,null,"クリプトンガス",6,6,"無"]
["ガラス","株式会社LIXIL","GLXC43N1","トリプルガラスグリーンxグリーンKrガス入り","G1",null,null,"クリプトンガス",6,6,"無"]
["ガラス","株式会社LIXIL","GLXC53N1","トリプルガラスクリアxグリーンKrガス入り","G1",null,null,"クリプトンガス",6,6,"無"]
["ガラス","株式会社LIXIL","GLXC63N1","トリプルガラスクリアxブロンズKrガス入り","G1",null,null,"クリプトンガス",6,6,"無"]
["ガラス","株式会社LIXIL","GLXC72N1","トリプルガラス一般xクリア(中空層Arガス入6)","G1",null,null,"アルゴンガス",6,6,"無"]
["ガラス","株式会社LIXIL","GLXC82N1","トリプルガラス一般xクリア(中空層Arガス入7以上)","G1",null,null,"アルゴンガス",7,7,"無"]
["ガラス","株式会社LIXIL","GLXC93N1","トリプルガラス一般xクリアKrガス入り","G1",null,null,"クリプトンガス",6,6,"無"]
["ガラス","株式会社LIXIL","GLXA21N2","Low-E複層ガラスクリア(中空層7～14)","G2",null,null,"乾燥空気",7,null,"無"]
["ガラス","株式会社LIXIL","GLXA41N2","Low-E複層ガラスグリーン(中空層7～13)","G2",null,null,"乾燥空気",7,null,"無"]
["ガラス","株式会社LIXIL","GLXA61N2","Low-E複層ガラスグリーン高遮熱仕様(中空層7～13)","G2",null,null,"乾燥空気",7,null,"無"]
["ガラス","株式会社LIXIL","GLXA62N2","Low-E複層ガラスクリア(中空層Arガス入8～10)","G2",null,null,"アルゴンガス",8,null,"無"]
["ガラス","株式会社LIXIL","GLXA81N2","Low-E複層ガラスブロンズ(中空層7～14)","G2",null,null,"乾燥空気",7,null,"無"]
["ガラス","株式会社LIXIL","GLXA82N2","Low-E複層ガラスグリーン(中空層Arガス入8～9)","G2",null,null,"アルゴンガス",8,null,"無"]
["ガラス","株式会社LIXIL","GLXA91Y2","AT付Low-E複層ガラスクリア(中空層7～12)","G2",null,null,"乾燥空気",7,null,"有"]
["ガラス","株式会社LIXIL","GLXB11Y2","AT付Low-E複層ガラスグリーン(中空層7～12)","G2",null,null,"乾燥空気",7,null,"有"]
["ガラス","株式会社LIXIL","GLXB12N2","Low-E複層ガラスグリーン高遮熱仕様(中空層Arガス入8～9)","G2",null,null,"アルゴンガス",8,null,"無"]
["ガラス","株式会社LIXIL","GLXB21Y2","AT付Low-E複層ガラスグリーン高遮熱仕様(中空層7～12)","G2",null,null,"乾燥空気",7,null,"有"]
["ガラス","株式会社LIXIL","GLXB31Y2","AT付Low-E複層ガラスブロンズ(中空層7～12)","G2",null,null,"乾燥空気",7,null,"有"]
["ガラス","株式会社LIXIL","GLXB32N2","Low-E複層ガラスブロンズ(中空層Arガス入8～10)","G2",null,null,"アルゴンガス",8,null,"無"]
["ガラス","株式会社LIXIL","GLXB52Y2","AT付Low-E複層ガラスクリア(中空層Arガス入8～10)","G2",null,null,"アルゴンガス",8,null,"有"]
["ガラス","株式会社LIXIL","GLXB72Y2","AT付Low-E複層ガラスグリーン(中空層Arガス入8～9)","G2",null,null,"アルゴンガス",8,null,"有"]
["ガラス","株式会社LIXIL","GLXB92Y2","AT付Low-E複層ガラスグリーン高遮熱仕様(中空層Arガス入8～9)","G2",null,null,"アルゴンガス",8,null,"有"]
["ガラス","株式会社LIXIL","GLXC22Y2","AT付Low-E複層ガラスブロンズ(中空層Arガス入8～10)","G2",null,null,"アルゴンガス",8,null,"有"]
["ガラス","YKK AP株式会社","GYK092N1","ｶﾞｽ入Low-E複層ガラス(遮熱ニュートラル)","G1",null,null,"アルゴンガス",12,null,"無"]
["ガラス","YKK AP株式会社","GYK101N1","Low-E複層ガラス(遮熱ブロンズ)","G1",null,null,"乾燥空気",15,null,"無"]
["ガラス","YKK AP株式会社","GYK102N1","ｶﾞｽ入Low-E複層ガラス(遮熱ブロンズ)","G1",null,null,"アルゴンガス",12,null,"無"]
["ガラス","YKK AP株式会社","GYKC12Y1","住宅引違い窓(ｶﾞﾗｽ溝9)用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(遮熱ﾌﾞﾙｰ)","G1",null,null,"アルゴンガス",11,null,"有"]
["ガラス","YKK AP株式会社","GYKC22Y1","住宅引違い窓(ｶﾞﾗｽ溝9)用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾙｰ)","G1",null,null,"アルゴンガス",11,null,"有"]
["ガラス","YKK AP株式会社","GYKC32Y1","住宅引違い窓(ｶﾞﾗｽ溝9)用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(断熱ﾆｭｰﾄﾗﾙ)","G1",null,null,"アルゴンガス",11,null,"有"]
["ガラス","YKK AP株式会社","GYKC42Y1","住宅引違い窓(ｶﾞﾗｽ溝9)用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾛﾝｽﾞ)","G1",null,null,"アルゴンガス",11,null,"有"]
["ガラス","YKK AP株式会社","GYKC52Y1","住宅FIX窓用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(遮熱ﾌﾞﾙｰ)","G1",null,null,"アルゴンガス",11,null,"有"]
["ガラス","YKK AP株式会社","GYKC62Y1","住宅FIX窓用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾙｰ)","G1",null,null,"アルゴンガス",11,null,"有"]
["ガラス","YKK AP株式会社","GYKC72Y1","住宅FIX窓用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(断熱ﾆｭｰﾄﾗﾙ)","G1",null,null,"アルゴンガス",11,null,"有"]
["ガラス","YKK AP株式会社","GYKC82Y1","住宅FIX窓用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾛﾝｽﾞ)","G1",null,null,"アルゴンガス",11,null,"有"]
["ガラス","YKK AP株式会社","GYKD12N1","マドリモAPW430用ｼﾝｸﾞﾙLow-E三層ガラス(ﾆｭｰﾄﾗﾙ)","G1",null,null,"アルゴンガス",14,14,"無"]
["ガラス","YKK AP株式会社","GYKD22N1","マドリモAPW430用ﾀﾞﾌﾞﾙLow-E三層ガラス(ﾌﾞﾙｰ)","G1",null,null,"アルゴンガス",14,14,"無"]
["ガラス","YKK AP株式会社","GYKD32N1","マドリモAPW430用ﾀﾞﾌﾞﾙLow-E三層ガラス(ﾆｭｰﾄﾗﾙ)","G1",null,null,"アルゴンガス",14,14,"無"]
["ガラス","YKK AP株式会社","GYKD42N1","マドリモAPW430用ﾀﾞﾌﾞﾙLow-E三層ガラス(ﾌﾞﾛﾝｽﾞ)","G1",null,null,"アルゴンガス",14,14,"無"]
["ガラス","YKK AP株式会社","GYKE11N1","Low-E複層ｶﾞﾗｽ(遮熱ﾌﾞﾙｰ)","G1",null,null,"乾燥空気",14,null,"無"]
["ガラス","YKK AP株式会社","GYKE21N1","Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾙｰ)","G1",null,null,"乾燥空気",14,null,"無"]
["ガラス","YKK AP株式会社","GYKE31N1","Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾛﾝｽﾞ)","G1",null,null,"乾燥空気",14,null,"無"]
["ガラス","YKK AP株式会社","GYKE41N1","Low-E複層ｶﾞﾗｽ(断熱ﾆｭｰﾄﾗﾙ)","G1",null,null,"乾燥空気",15,null,"無"]
["ガラス","YKK AP株式会社","GYKE51N1","Low-E複層ｶﾞﾗｽ(遮熱ﾆｭｰﾄﾗﾙ)","G1",null,null,"乾燥空気",15,null,"無"]
["ガラス","YKK AP株式会社","GYKF12N1","ｶﾞｽ入Low-E複層ｶﾞﾗｽ(遮熱ﾌﾞﾙｰ)","G1",null,null,"アルゴンガス",10,null,"無"]
["ガラス","YKK AP株式会社","GYKF22N1","ｶﾞｽ入Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾙｰ)","G1",null,null,"アルゴンガス",10,null,"無"]
["ガラス","YKK AP株式会社","GYKF32N1","ｶﾞｽ入Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾛﾝｽﾞ)","G1",null,null,"アルゴンガス",10,null,"無"]
["ガラス","YKK AP株式会社","GYKF42N1","ｶﾞｽ入Low-E複層ｶﾞﾗｽ(断熱ﾆｭｰﾄﾗﾙ)","G1",null,null,"アルゴンガス",11,null,"無"]
["ガラス","YKK AP株式会社","GYK011N2","Low-E複層ガラス(遮熱ブルー)","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","YKK AP株式会社","GYK011Y2","ビル引違い窓(ｶﾞﾗｽ溝13、14)用ｱﾀｯﾁﾒﾝﾄ付Low-E複層ｶﾞﾗｽ(遮熱ﾌﾞﾙｰ)","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","YKK AP株式会社","GYK012N2","ｶﾞｽ入Low-E複層ガラス(遮熱ブルー)","G2",null,null,"アルゴンガス",6,null,"無"]
["ガラス","YKK AP株式会社","GYK012Y2","ﾋﾞﾙ引違い窓(ｶﾞﾗｽ溝13、14)用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(遮熱ﾌﾞﾙｰ)","G2",null,null,"アルゴンガス",6,null,"有"]
["ガラス","YKK AP株式会社","GYK021Y2","ビル引違い窓(ｶﾞﾗｽ溝13、14)用ｱﾀｯﾁﾒﾝﾄ付Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾙｰ)","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","YKK AP株式会社","GYK022Y2","ﾋﾞﾙ引違い窓(ｶﾞﾗｽ溝13、14)用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾙｰ)","G2",null,null,"アルゴンガス",6,null,"有"]
["ガラス","YKK AP株式会社","GYK031N2","Low-E複層ガラス(断熱ブルー)","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","YKK AP株式会社","GYK031Y2","ビル引違い窓(ｶﾞﾗｽ溝13、14)用ｱﾀｯﾁﾒﾝﾄ付Low-E複層ｶﾞﾗｽ(断熱ﾆｭｰﾄﾗﾙ)","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","YKK AP株式会社","GYK032N2","ｶﾞｽ入Low-E複層ガラス(断熱ブルー)","G2",null,null,"アルゴンガス",6,null,"無"]
["ガラス","YKK AP株式会社","GYK032Y2","ﾋﾞﾙ引違い窓(ｶﾞﾗｽ溝13、14)用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(断熱ニュートラル)","G2",null,null,"アルゴンガス",6,null,"有"]
["ガラス","YKK AP株式会社","GYK041Y2","ビル引違い窓(ｶﾞﾗｽ溝13、14)用ｱﾀｯﾁﾒﾝﾄ付Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾛﾝｽﾞ)","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","YKK AP株式会社","GYK042Y2","ﾋﾞﾙ引違い窓(ｶﾞﾗｽ溝13、14)用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾛﾝｽﾞ)","G2",null,null,"アルゴンガス",6,null,"有"]
["ガラス","YKK AP株式会社","GYK051N2","Low-E複層ガラス(断熱ニュートラル)","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","YKK AP株式会社","GYK051Y2","ﾋﾞﾙFIX窓(ｶﾞﾗｽ溝13、14)用ｱﾀｯﾁﾒﾝﾄ付Low-E複層ｶﾞﾗｽ(遮熱ﾌﾞﾙｰ)","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","YKK AP株式会社","GYK052N2","ｶﾞｽ入Low-E複層ガラス(断熱ニュートラル)","G2",null,null,"アルゴンガス",6,null,"無"]
["ガラス","YKK AP株式会社","GYK052Y2","ﾋﾞﾙFIX窓(ｶﾞﾗｽ溝13、14)用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(遮熱ﾌﾞﾙｰ)","G2",null,null,"アルゴンガス",6,null,"有"]
["ガラス","YKK AP株式会社","GYK061N2","Low-E複層ガラス(断熱ブロンズ)","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","YKK AP株式会社","GYK061Y2","ﾋﾞﾙFIX窓(ｶﾞﾗｽ溝13、14)用ｱﾀｯﾁﾒﾝﾄ付Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾙｰ)","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","YKK AP株式会社","GYK062Y2","ﾋﾞﾙFIX窓(ｶﾞﾗｽ溝13、14)用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾙｰ)","G2",null,null,"アルゴンガス",6,null,"有"]
["ガラス","YKK AP株式会社","GYK071Y2","ﾋﾞﾙFIX窓(ｶﾞﾗｽ溝13、14)用ｱﾀｯﾁﾒﾝﾄ付Low-E複層ｶﾞﾗｽ(断熱ﾆｭｰﾄﾗﾙ)","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","YKK AP株式会社","GYK072N2","ｶﾞｽ入Low-E複層ガラス(断熱ブロンズ)","G2",null,null,"アルゴンガス",6,null,"無"]
["ガラス","YKK AP株式会社","GYK072Y2","ﾋﾞﾙFIX窓(ｶﾞﾗｽ溝13、14)用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(断熱ﾆｭｰﾄﾗﾙ)","G2",null,null,"アルゴンガス",6,null,"有"]
["ガラス","YKK AP株式会社","GYK081N2","Low-E複層ガラス(遮熱ニュートラル)","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","YKK AP株式会社","GYK081Y2","ﾋﾞﾙFIX窓(ｶﾞﾗｽ溝13、14)用ｱﾀｯﾁﾒﾝﾄ付Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾛﾝｽﾞ)","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","YKK AP株式会社","GYK082Y2","ﾋﾞﾙFIX窓(ｶﾞﾗｽ溝13、14)用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾛﾝｽﾞ)","G2",null,null,"アルゴンガス",6,null,"有"]
["ガラス","YKK AP株式会社","GYK091N2","Low-E複層ガラス(遮熱ブロンズ)","G2",null,null,"乾燥空気",8,null,"無"]
["ガラス","YKK AP株式会社","GYK091Y2","ビル引違い窓(ｶﾞﾗｽ溝13、14)用ｱﾀｯﾁﾒﾝﾄ付Low-E複層ｶﾞﾗｽ(遮熱ニュートラル)","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","YKK AP株式会社","GYK101Y2","ビル引違い窓(ｶﾞﾗｽ溝13、14)用ｱﾀｯﾁﾒﾝﾄ付Low-E複層ｶﾞﾗｽ(遮熱ブロンズ)","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","YKK AP株式会社","GYK111Y2","ﾋﾞﾙFIX窓(ｶﾞﾗｽ溝13、14)用ｱﾀｯﾁﾒﾝﾄ付Low-E複層ｶﾞﾗｽ(遮熱ﾆｭｰﾄﾗﾙ)","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","YKK AP株式会社","GYK121Y2","ﾋﾞﾙFIX窓(ｶﾞﾗｽ溝13、14)用ｱﾀｯﾁﾒﾝﾄ付Low-E複層ｶﾞﾗｽ(遮熱ﾌﾞﾛﾝｽﾞ)","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","YKK AP株式会社","GYKA11Y2","住宅引違い窓(ｶﾞﾗｽ溝9)用ｱﾀｯﾁﾒﾝﾄ付Low-E複層ｶﾞﾗｽ(遮熱ﾌﾞﾙｰ)","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","YKK AP株式会社","GYKA21Y2","住宅引違い窓(ｶﾞﾗｽ溝9)用ｱﾀｯﾁﾒﾝﾄ付Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾙｰ)","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","YKK AP株式会社","GYKA31Y2","住宅引違い窓(ｶﾞﾗｽ溝9)用ｱﾀｯﾁﾒﾝﾄ付Low-E複層ｶﾞﾗｽ(断熱ﾆｭｰﾄﾗﾙ)","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","YKK AP株式会社","GYKA41Y2","住宅引違い窓(ｶﾞﾗｽ溝9)用ｱﾀｯﾁﾒﾝﾄ付Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾛﾝｽﾞ)","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","YKK AP株式会社","GYKA51Y2","住宅FIX窓用ｱﾀｯﾁﾒﾝﾄ付Low-E複層ｶﾞﾗｽ(遮熱ﾌﾞﾙｰ)","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","YKK AP株式会社","GYKA61Y2","住宅FIX窓用ｱﾀｯﾁﾒﾝﾄ付Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾙｰ)","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","YKK AP株式会社","GYKA71Y2","住宅FIX窓用ｱﾀｯﾁﾒﾝﾄ付Low-E複層ｶﾞﾗｽ(断熱ﾆｭｰﾄﾗﾙ)","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","YKK AP株式会社","GYKA81Y2","住宅FIX窓用ｱﾀｯﾁﾒﾝﾄ付Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾛﾝｽﾞ)","G2",null,null,"乾燥空気",8,null,"有"]
["ガラス","YKK AP株式会社","GYKB12Y2","住宅引違い窓(ｶﾞﾗｽ溝9)用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(遮熱ﾌﾞﾙｰ)","G2",null,null,"アルゴンガス",5,null,"有"]
["ガラス","YKK AP株式会社","GYKB22Y2","住宅引違い窓(ｶﾞﾗｽ溝9)用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾙｰ)","G2",null,null,"アルゴンガス",5,null,"有"]
["ガラス","YKK AP株式会社","GYKB32Y2","住宅引違い窓(ｶﾞﾗｽ溝9)用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(断熱ﾆｭｰﾄﾗﾙ)","G2",null,null,"アルゴンガス",5,null,"有"]
["ガラス","YKK AP株式会社","GYKB42Y2","住宅引違い窓(ｶﾞﾗｽ溝9)用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾛﾝｽﾞ)","G2",null,null,"アルゴンガス",5,null,"有"]
["ガラス","YKK AP株式会社","GYKB52Y2","住宅FIX窓用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(遮熱ﾌﾞﾙｰ)","G2",null,null,"アルゴンガス",5,null,"有"]
["ガラス","YKK AP株式会社","GYKB62Y2","住宅FIX窓用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾙｰ)","G2",null,null,"アルゴンガス",5,null,"有"]
["ガラス","YKK AP株式会社","GYKB72Y2","住宅FIX窓用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(断熱ﾆｭｰﾄﾗﾙ)","G2",null,null,"アルゴンガス",5,null,"有"]
["ガラス","YKK AP株式会社","GYKB82Y2","住宅FIX窓用ｱﾀｯﾁﾒﾝﾄ付ｶﾞｽ入Low-E複層ｶﾞﾗｽ(断熱ﾌﾞﾛﾝｽﾞ)","G2",null,null,"アルゴンガス",5,null,"有"]
["窓","アイパワーフォレスト株式会社","W437A1225","木製引き違いインナーサッシ　W","W5",null,null,null,null,null,null,"木製・内窓",16,null,null,null,"Low-E複層","アルゴンガス"]
["窓","アルス株式会社","W122D1421","YMﾄﾞﾚｰキップ90","W1",null,null,null,null,null,null,"木製・外窓",16,16,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","アルス株式会社","W122F1213","YMFIX56","W3",null,null,null,null,null,null,"木製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","アルス株式会社","W122H1214","YMﾍｰﾍﾞｼｰﾍﾞ56","W4",null,null,null,null,null,null,"木製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","アルス株式会社","W122H2214","YMﾍｰﾍﾞｼｰﾍﾞ2枚引き込み56","W4",null,null,null,null,null,null,"木製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","アルス株式会社","W122O1214","YM片開きドア56","W4",null,null,null,null,null,null,"木製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","アルメタックス株式会社","W096B1245","あるまど(内窓)内開き","W5",null,null,null,null,null,null,"樹脂製・内窓",0.2,null,null,null,"Low-E複層","真空"]
["窓","アルメタックス株式会社","W096H1215","あるまど(内窓)　引き違い","W5",null,null,null,null,null,null,"樹脂製・内窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社ウッドワン","W157A1215","MOKUサッシ　Low-E透明ガラス(遮熱タイプ)","W5",null,null,null,null,null,null,"木製・内窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社ウッドワン","W157A2215","MOKUサッシ　Low-E透明ガラス(断熱タイプ)","W5",null,null,null,null,null,null,"木製・内窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社ウッドワン","W157A3145","MOKUサッシ　薄型断熱ガラス(透明)","W5",null,null,null,null,null,null,"木製・内窓",0.2,null,null,null,"複層","真空"]
["窓","株式会社ウッドワン","W157A4115","MOKUサッシ　透明ガラス","W5",null,null,null,null,null,null,"木製・内窓",12,null,null,null,"複層","乾燥空気"]
["窓","株式会社ウッドワン","W157A8115","MOKUサッシ　内開きテラス窓　透明ガラス","W5",null,null,null,null,null,null,"木製・内窓",12,null,null,null,"複層","乾燥空気"]
["窓","株式会社ウッドワン","W157B3145","MOKUサッシ　薄型断熱ガラス(すり板)","W5",null,null,null,null,null,null,"木製・内窓",0.2,null,null,null,"複層","真空"]
["窓","株式会社ウッドワン","W157B7145","MOKUサッシ　　内開きテラス窓　薄型断熱ガラスすり板","W5",null,null,null,null,null,null,"木製・内窓",0.2,null,null,null,"複層","真空"]
["窓","株式会社ウッドワン","W157C1215","MOKUサッシ　Low-E型ガラス(遮熱タイプ)","W5",null,null,null,null,null,null,"木製・内窓",11,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社ウッドワン","W157C2215","MOKUサッシ　Low-E型ガラス(断熱タイプ)","W5",null,null,null,null,null,null,"木製・内窓",11,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社ウッドワン","W157C5215","MOKUサッシ　内開きテラス窓　Low-E型ガラス遮熱タイプ","W5",null,null,null,null,null,null,"木製・内窓",11,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社エクセルシャノン","W051A2421","ｼｬﾉﾝｳｲﾝﾄﾞUFｼﾘｰｽﾞ【UF-H】 ダブルLow-E(Ar)","W1",null,null,null,null,null,null,"樹脂製・外窓",9,9,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社エクセルシャノン","W051B2421","ｼｬﾉﾝｳｲﾝﾄﾞUFｼﾘｰｽﾞ【UF-L】　ダブルLow-E(Ar)","W1",null,null,null,null,null,null,"樹脂製・外窓",9,9,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社エクセルシャノン","W051K2422","トリプルシャノンIIx　ダブルLow-E(Ar)テラスドアN(パネル仕様を除く)","W2",null,null,null,null,null,null,"樹脂製・外窓",13.5,13.5,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社エクセルシャノン","W051K3422","トリプルシャノンIIx ダブルLow-E(Ar)テラスドア(パネル仕様を除く)","W2",null,null,null,null,null,null,"樹脂製・外窓",13.5,13.5,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社エクセルシャノン","W051A1213","ｼｬﾉﾝｳｲﾝﾄﾞUFｼﾘｰｽﾞ【UF-H】 Low-E","W3",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社エクセルシャノン","W051A3223","ｼｬﾉﾝｳｲﾝﾄﾞUFｼﾘｰｽﾞ【UF-H】 Low-E(Ar)","W3",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社エクセルシャノン","W051B3223","ｼｬﾉﾝｳｲﾝﾄﾞUFｼﾘｰｽﾞ【UF-L】　Low-E(Ar)","W3",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社エクセルシャノン","W051D4223","シャノンウインドRI　Low-E(Ar)(防火窓)","W3",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社エクセルシャノン","W051E3223","シャノンウインドTypeEB　Low-E(Ar)","W3",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社エクセルシャノン","W051F1423","トリプルシャノンIIs　ダブルLow-E(Ar)","W3",null,null,null,null,null,null,"樹脂製・外窓",7.5,7.5,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社エクセルシャノン","W051H2223","シャノンウインドRI　Low-E(Ar)テラスドアN(パネル仕様を除く)","W3",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社エクセルシャノン","W051I3223","シャノンウインドTypeEB　Low-E(Ar)テラスドア","W3",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社エクセルシャノン","W051J1423","トリプルシャノンIIs　ダブルLow-E(Ar)テラスドア(パネル仕様を除く)","W3",null,null,null,null,null,null,"樹脂製・外窓",7.5,7.5,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社エクセルシャノン","W051J2423","トリプルシャノンIIs　ダブルLow-E(Ar)テラスドアN(パネル仕様を除く)","W3",null,null,null,null,null,null,"樹脂製・外窓",7.5,7.5,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社エクセルシャノン","W051K1423","トリプルシャノンIIx　ダブルLow-E(Ar)","W3",null,null,null,null,null,null,"樹脂製・外窓",8,10,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社エクセルシャノン","W051B1214","ｼｬﾉﾝｳｲﾝﾄﾞUFｼﾘｰｽﾞ【UF-L】　Low-E","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社エクセルシャノン","W051C1224","シャノンウインドIIs　Low-E(Ar)","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社エクセルシャノン","W051C2214","シャノンウインドIIs　Low-E","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社エクセルシャノン","W051D1214","シャノンウインドRI　Low-E","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社エクセルシャノン","W051D2214","シャノンウインドRI　Low-E(防火窓)","W4",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社エクセルシャノン","W051D3224","シャノンウインドRI　Low-E(Ar)","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社エクセルシャノン","W051E1214","シャノンウインドTypeEB　Low-E","W4",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社エクセルシャノン","W051G1224","シャノンウインドIIs　Low-E(Ar)テラスドア(パネル仕様を除く)","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社エクセルシャノン","W051G2224","シャノンウインドIIs　Low-E(Ar)テラスドアN(パネル仕様を除く)","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社エクセルシャノン","W051G3214","シャノンウインドIIs　Low-Eテラスドア(パネル仕様を除く)","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社エクセルシャノン","W051G4214","シャノンウインドIIs　Low-EテラスドアN(パネル仕様を除く)","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社エクセルシャノン","W051H1214","シャノンウインドRI　Low-EテラスドアN(パネル仕様を除く)","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社エクセルシャノン","W051I1214","シャノンウインドTypeEB　Low-Eテラスドア","W4",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","乾燥空気"]
["窓","AGC株式会社","W066P2215","まどまど　plus　Low-E","W5",null,null,null,null,null,null,"樹脂製・内窓",6,null,null,null,"Low-E複層","乾燥空気"]
["窓","AGC株式会社","W066P3225","まどまど　plus　Low-E(Ar)","W5",null,null,null,null,null,null,"樹脂製・内窓",6,null,null,null,"Low-E複層","アルゴンガス"]
["窓","AGC株式会社","W066S1115","まどまど　std","W5",null,null,null,null,null,null,"樹脂製・内窓",6,null,null,null,"複層","乾燥空気"]
["窓","AGC株式会社","W066S2215","まどまど　std　Low-E","W5",null,null,null,null,null,null,"樹脂製・内窓",4,null,null,null,"Low-E複層","乾燥空気"]
["窓","AGC株式会社","W066S3225","まどまど　std　Low-E(Ar)","W5",null,null,null,null,null,null,"樹脂製・内窓",4,null,null,null,"Low-E複層","アルゴンガス"]
["窓","AGC株式会社","W066S4115","まどまど　std　テラスドア","W5",null,null,null,null,null,null,"樹脂製・内窓",6,null,null,null,"複層","乾燥空気"]
["窓","AGC株式会社","W066S5215","まどまど　std　テラスドア　Low-E","W5",null,null,null,null,null,null,"樹脂製・内窓",4,null,null,null,"Low-E複層","乾燥空気"]
["窓","AGC株式会社","W066S6225","まどまど　std　テラスドア　Low-E(Ar)","W5",null,null,null,null,null,null,"樹脂製・内窓",4,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社キムラ","W422A1421","ヴィージェイ・フェンスター　木製断熱窓","W1",null,null,null,null,null,null,"木製・外窓",15,15,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社栗原","W226U1225","K-WINDOW内窓 Low-E(Ar)","W5",null,null,null,null,null,null,"樹脂製・内窓",15,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社栗原","W226U2425","K-WINDOW内窓 トリプル25(Ar)","W5",null,null,null,null,null,null,"樹脂製・内窓",8,8,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社栗原","W226U3425","K-WINDOW内窓 トリプル35(Ar)","W5",null,null,null,null,null,null,"樹脂製・内窓",12,12,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社栗原","W226U4425","K-WINDOW内窓 トリプル44(Ar)","W5",null,null,null,null,null,null,"樹脂製・内窓",16,16,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社栗原","W221K5421","K-WINDOW　2×6枠　トリプル(Ar)","W1",null,null,null,null,null,null,"樹脂製・外窓",12,12,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社栗原","W221K6421","K-WINDOW　トリプル(Ar)","W1",null,null,null,null,null,null,"樹脂製・外窓",12,12,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社栗原","W221K8421","K-WINDOW　テラスドア　トリプル41(Ar)","W1",null,null,null,null,null,null,"樹脂製・外窓",16,16,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社栗原","W221K3222","K-WINDOW　テラスドア　LOW-Eぺア(Ar)","W2",null,null,null,null,null,null,"樹脂製・外窓",15,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社栗原","W221K4422","K-WINDOW　トリプル25(Ar)","W2",null,null,null,null,null,null,"樹脂製・外窓",8,8,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社栗原","W221K2223","K-WINDOW　LOW-E(Ar)","W3",null,null,null,null,null,null,"樹脂製・外窓",15,null,null,null,"Low-E複層","アルゴンガス"]
["窓","クレトイシ株式会社","W261M1223","montage","W3",null,null,null,null,null,null,"樹脂製・外窓",10,null,null,null,"Low-E複層","アルゴンガス"]
["窓","クレトイシ株式会社","W261M2423","montage　トリプルガラス","W3",null,null,null,null,null,null,"樹脂製・外窓",8,8,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","クレトイシ株式会社","W261M3223","montage　防火窓","W3",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W01DZ1226","アルジオBv","W6",null,null,null,null,null,null,"アルミ樹脂複合製・カバー(ビル用)",16,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W011Y1422","ﾄﾘﾌﾟﾙｱﾙﾍﾟﾝIIx","W2",null,null,null,null,null,null,"樹脂製・外窓",9.5,9.5,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","三協立山株式会社","W011Y2422","ﾄﾘﾌﾟﾙｱﾙﾍﾟﾝIIxﾃﾗｽﾄﾞｱ","W2",null,null,null,null,null,null,"樹脂製・外窓",9.5,9.5,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","三協立山株式会社","W011Y3422","ﾄﾘﾌﾟﾙｱﾙﾍﾟﾝIIx勝手口ドア(中さん無)","W2",null,null,null,null,null,null,"樹脂製・外窓",9.5,9.5,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","三協立山株式会社","W011Y4223","ｱﾙﾍﾟﾝIIs","W3",null,null,null,null,null,null,"樹脂製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W011Y5223","ｱﾙﾍﾟﾝIIsﾃﾗｽﾄﾞｱ","W3",null,null,null,null,null,null,"樹脂製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W011Y6223","ｱﾙﾍﾟﾝIIs勝手口ﾄﾞｱ(中さん無)","W3",null,null,null,null,null,null,"樹脂製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W011Y7224","ｱﾙﾍﾟﾝIIs(CVDｸﾘｱ)","W4",null,null,null,null,null,null,"樹脂製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W011Y8224","ｱﾙﾍﾟﾝIIs(CVDｸﾘｱ)ﾃﾗｽﾄﾞｱ","W4",null,null,null,null,null,null,"樹脂製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W011Y9224","ｱﾙﾍﾟﾝIIs(CVDｸﾘｱ)勝手口ﾄﾞｱ(中さん無)","W4",null,null,null,null,null,null,"樹脂製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W011D5431","ﾄﾘﾌﾟﾙｽﾏｰｼﾞｭ","W1",null,null,null,null,null,null,"樹脂製・外窓",8,8,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","三協立山株式会社","W011D6431","ﾄﾘﾌﾟﾙｽﾏｰｼﾞｭﾃﾗｽﾄﾞｱ","W1",null,null,null,null,null,null,"樹脂製・外窓",8,8,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","三協立山株式会社","W011D7431","ﾄﾘﾌﾟﾙｽﾏｰｼﾞｭ勝手口ﾄﾞｱ中無","W1",null,null,null,null,null,null,"樹脂製・外窓",8,8,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","三協立山株式会社","W011P1222","ｽﾏｰｼﾞｭ","W2",null,null,null,null,null,null,"樹脂製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W011P2222","ｽﾏｰｼﾞｭﾃﾗｽﾄﾞｱ","W2",null,null,null,null,null,null,"樹脂製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W011P3222","ｽﾏｰｼﾞｭ勝手口ﾄﾞｱ中無","W2",null,null,null,null,null,null,"樹脂製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W013U1422","ｱﾙｼﾞｵLow-Eﾄﾘﾌﾟﾙ(Ar)","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",10,10,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","三協立山株式会社","W013U2422","ｱﾙｼﾞｵﾃﾗｽﾄﾞｱLow-Eﾄﾘﾌﾟﾙ(Ar)","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",10,10,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","三協立山株式会社","W013U3422","ｱﾙｼﾞｵ勝手口ﾄﾞｱ中無(採風除く)Low-Eﾄﾘﾌﾟﾙ(Ar)","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",10,10,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","三協立山株式会社","W013U4422","ｱﾙｼﾞｵ勝手口ﾄﾞｱ中付(採風除く)Low-Eﾄﾘﾌﾟﾙ(Ar)","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",10,10,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","三協立山株式会社","W01AX1222","ﾘﾌｫｰﾑｽﾏｰｼﾞｭ","W2",null,null,null,null,null,null,"樹脂製・カバー(住宅用)",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W013K5223","ﾏﾃﾞｨｵJ Low-E(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W013K6223","ﾏﾃﾞｨｵJﾃﾗｽﾄﾞｱLow-E(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W013K7223","ﾏﾃﾞｨｵJ勝手口ﾄﾞｱ中無(採風除く)Low-E(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W013K8223","ﾏﾃﾞｨｵJ勝手口ﾄﾞｱ中付(採風除く)Low-E(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W013O1443","ｱﾙｼﾞｵLow-E真空","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",9,0.2,null,null,"ダブルLow-E三層","真空"]
["窓","三協立山株式会社","W013O2443","ｱﾙｼﾞｵﾃﾗｽﾄﾞｱLow-E真空","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",9,0.2,null,null,"ダブルLow-E三層","真空"]
["窓","三協立山株式会社","W013O3443","ｱﾙｼﾞｵ勝手口ﾄﾞｱ中無(採風除く)Low-E真空","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",9,0.2,null,null,"ダブルLow-E三層","真空"]
["窓","三協立山株式会社","W013O4443","ｱﾙｼﾞｵ勝手口ﾄﾞｱ中付(採風除く)Low-E真空","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",9,0.2,null,null,"ダブルLow-E三層","真空"]
["窓","三協立山株式会社","W013Q1223","ｱﾙｼﾞｵLow-E(Ar)","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W013Q2223","ｱﾙｼﾞｵﾃﾗｽﾄﾞｱLow-E(Ar)","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W013Q3223","ｱﾙｼﾞｵ勝手口ﾄﾞｱ中無(採風除く)Low-E(Ar)","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W013Q4223","ｱﾙｼﾞｵ勝手口ﾄﾞｱ中付(採風除く)Low-E(Ar)","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W013V1223","ﾏﾃﾞｨｵM Low-E(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W013A1214","ｱﾙｼﾞｵLow-E","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","三協立山株式会社","W013A2214","ｱﾙｼﾞｵﾃﾗｽﾄﾞｱLow-E","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","三協立山株式会社","W013A3214","ｱﾙｼﾞｵ勝手口ﾄﾞｱ中付(採風除く)Low-E","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","三協立山株式会社","W013A4214","ｱﾙｼﾞｵ勝手口ﾄﾞｱ中無(採風除く)Low-E","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","三協立山株式会社","W013G1214","防火窓ｱﾙｼﾞｵLow-E","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","三協立山株式会社","W013G2214","防火窓ｱﾙｼﾞｵﾃﾗｽﾄﾞｱLow-E","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","三協立山株式会社","W013G3214","防火窓ｱﾙｼﾞｵ勝手口ﾄﾞｱ(採風除く)Low-E","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","三協立山株式会社","W013H1224","防火窓ｱﾙｼﾞｵLow-E(Ar)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W013H2224","防火窓ｱﾙｼﾞｵﾃﾗｽﾄﾞｱLow-E(Ar)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W013H3224","防火窓ｱﾙｼﾞｵ勝手口ﾄﾞｱ(採風除く)Low-E(Ar)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W013K1224","ﾏﾃﾞｨｵJ Low-E(Ar)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W013K2224","ﾏﾃﾞｨｵJﾃﾗｽﾄﾞｱLow-E(Ar)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W013K3224","ﾏﾃﾞｨｵJ勝手口ドア中付(採風除く)Low-E(Ar)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W013K4224","ﾏﾃﾞｨｵJ勝手口ﾄﾞｱ中無(採風除く)Low-E(Ar)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W013L1214","ﾏﾃﾞｨｵJ Low-E","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","三協立山株式会社","W013L2214","ﾏﾃﾞｨｵJﾃﾗｽﾄﾞｱLow-E","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","三協立山株式会社","W013L3214","ﾏﾃﾞｨｵJ勝手口ドア中付(採風除く)Low-E","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","三協立山株式会社","W013L4214","ﾏﾃﾞｨｵJ勝手口ﾄﾞｱ中無(採風除く)Low-E","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","三協立山株式会社","W013M1224","ﾏﾃﾞｨｵM Low-E(Ar)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W013N1214","ﾏﾃﾞｨｵM Low-E","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","三協立山株式会社","W013T1224","防火ｻｯｼF型ｱﾙﾐ樹脂複合ﾀｲﾌﾟLow-E(Ar)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",10,null,null,null,"Low-E複層","アルゴンガス"]
["窓","三協立山株式会社","W016E1115","ﾌﾟﾗﾒｲｸ","W5",null,null,null,null,null,null,"樹脂製・内窓",10,null,null,null,"複層","乾燥空気"]
["窓","三協立山株式会社","W016E2215","ﾌﾟﾗﾒｲｸLow-E","W5",null,null,null,null,null,null,"樹脂製・内窓",10,null,null,null,"Low-E複層","乾燥空気"]
["窓","三協立山株式会社","W016E3145","ﾌﾟﾗﾒｲｸ真空","W5",null,null,null,null,null,null,"樹脂製・内窓",0.2,null,null,null,"複層","真空"]
["窓","三協立山株式会社","W016F1115","ﾌﾟﾗﾒｲｸE2","W5",null,null,null,null,null,null,"樹脂製・内窓",10,null,null,null,"複層","乾燥空気"]
["窓","三協立山株式会社","W016F2215","ﾌﾟﾗﾒｲｸE2Low-E","W5",null,null,null,null,null,null,"樹脂製・内窓",10,null,null,null,"Low-E複層","乾燥空気"]
["窓","三協立山株式会社","W016F3145","ﾌﾟﾗﾒｲｸE2真空","W5",null,null,null,null,null,null,"樹脂製・内窓",0.2,null,null,null,"複層","真空"]
["窓","三協立山株式会社","W016F4115","ﾌﾟﾗﾒｲｸE2ﾃﾗｽﾄﾞｱ","W5",null,null,null,null,null,null,"樹脂製・内窓",10,null,null,null,"複層","乾燥空気"]
["窓","三協立山株式会社","W016F5215","ﾌﾟﾗﾒｲｸE2ﾃﾗｽﾄﾞｱLow-E","W5",null,null,null,null,null,null,"樹脂製・内窓",10,null,null,null,"Low-E複層","乾燥空気"]
["窓","三協立山株式会社","W016F6145","ﾌﾟﾗﾒｲｸE2ﾃﾗｽﾄﾞｱ真空","W5",null,null,null,null,null,null,"樹脂製・内窓",0.2,null,null,null,"複層","真空"]
["窓","三協立山株式会社","W016F7115","ﾌﾟﾗﾒｲｸE2内窓ブレス付DI窓","W5",null,null,null,null,null,null,"樹脂製・内窓",12,null,null,null,"複層","乾燥空気"]
["窓","スウェーデンハウス株式会社","W322B1313","バルコニードア(BD)","W3",null,null,null,null,null,null,"木製・外窓",12,12,null,null,"Low-E三層","乾燥空気"]
["窓","スウェーデンハウス株式会社","W322B2313","バルコニードア(FBD)","W3",null,null,null,null,null,null,"木製・外窓",12,12,null,null,"Low-E三層","乾燥空気"]
["窓","スウェーデンハウス株式会社","W322B3313","バルコニードア(FCBD)","W3",null,null,null,null,null,null,"木製・外窓",12,12,null,null,"Low-E三層","乾燥空気"]
["窓","スウェーデンハウス株式会社","W322B4313","バルコニードア(SBD)","W3",null,null,null,null,null,null,"木製・外窓",12,12,null,null,"Low-E三層","乾燥空気"]
["窓","スウェーデンハウス株式会社","W322B5313","両開きバルコニードア","W3",null,null,null,null,null,null,"木製・外窓",12,12,null,null,"Low-E三層","乾燥空気"]
["窓","スウェーデンハウス株式会社","W322W1313","木製サッシ三層ガラス窓","W3",null,null,null,null,null,null,"木製・外窓",12,12,null,null,"Low-E三層","乾燥空気"]
["窓","大信工業株式会社","W086D1115","内窓プラスト　一般複層","W5",null,null,null,null,null,null,"樹脂製・内窓",12,null,null,null,"複層","乾燥空気"]
["窓","大信工業株式会社","W086D2215","内窓プラスト　Low-E　A6","W5",null,null,null,null,null,null,"樹脂製・内窓",6,null,null,null,"Low-E複層","乾燥空気"]
["窓","大信工業株式会社","W086D4225","内窓プラスト　Low-Eガス入　A6","W5",null,null,null,null,null,null,"樹脂製・内窓",6,null,null,null,"Low-E複層","アルゴンガス"]
["窓","大信工業株式会社","W086D6245","内窓プラスト　スペーシア","W5",null,null,null,null,null,null,"樹脂製・内窓",0.2,null,null,null,"Low-E複層","真空"]
["窓","大信工業株式会社","W086D7145","内窓プラスト　クリアフィット","W5",null,null,null,null,null,null,"樹脂製・内窓",0.2,null,null,null,"複層","真空"]
["窓","大信工業株式会社","W086K1115","内窓プラストKR　一般複層","W5",null,null,null,null,null,null,"樹脂製・内窓",6,null,null,null,"複層","乾燥空気"]
["窓","大信工業株式会社","W086K2245","内窓プラストKR　スペーシア","W5",null,null,null,null,null,null,"樹脂製・内窓",0.2,null,null,null,"Low-E複層","真空"]
["窓","大信工業株式会社","W086K3145","内窓プラストKR　クリアフィット","W5",null,null,null,null,null,null,"樹脂製・内窓",0.2,null,null,null,"複層","真空"]
["窓","日昭株式会社","W106E1115","ｴｺｳｨﾝﾄﾞ","W5",null,null,null,null,null,null,"樹脂製・内窓",10,null,null,null,"複層","乾燥空気"]
["窓","日昭株式会社","W106E2215","ｴｺｳｨﾝﾄﾞLow-E","W5",null,null,null,null,null,null,"樹脂製・内窓",10,null,null,null,"Low-E複層","乾燥空気"]
["窓","日昭株式会社","W106E3145","ｴｺｳｨﾝﾄﾞ真空","W5",null,null,null,null,null,null,"樹脂製・内窓",0.2,null,null,null,"複層","真空"]
["窓","日昭株式会社","W106E4115","ｴｺｳｨﾝﾄﾞﾃﾗｽﾄﾞｱ","W5",null,null,null,null,null,null,"樹脂製・内窓",10,null,null,null,"複層","乾燥空気"]
["窓","日昭株式会社","W106E5215","ｴｺｳｨﾝﾄﾞﾃﾗｽﾄﾞｱLow-E","W5",null,null,null,null,null,null,"樹脂製・内窓",10,null,null,null,"Low-E複層","乾燥空気"]
["窓","日昭株式会社","W106E6145","ｴｺｳｨﾝﾄﾞﾃﾗｽﾄﾞｱ真空","W5",null,null,null,null,null,null,"樹脂製・内窓",0.2,null,null,null,"複層","真空"]
["窓","株式会社日本の窓","W442L3431","MADOBA　W-LowE(Kr)","W1",null,null,null,null,null,null,"木製・外窓",12,12,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社日本の窓","W442L1412","MADOBA　W-LowE","W2",null,null,null,null,null,null,"木製・外窓",12,12,null,null,"ダブルLow-E三層","乾燥空気"]
["窓","株式会社日本の窓","W442L2422","MADOBA　W-LowE(Ar)","W2",null,null,null,null,null,null,"木製・外窓",12,12,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社日本の窓","W442T1312","MADOBA　トリプル","W2",null,null,null,null,null,null,"木製・外窓",12,12,null,null,"Low-E三層","乾燥空気"]
["窓","株式会社日本の窓","W442T2322","MADOBA　トリプル(Ar)","W2",null,null,null,null,null,null,"木製・外窓",12,12,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社日本の窓","W442T3332","MADOBA　トリプル(Kr)","W2",null,null,null,null,null,null,"木製・外窓",12,12,null,null,"Low-E三層","クリプトンガス"]
["窓","株式会社日本の窓","W442W2222","MADOBA　ペア(Ar)","W2",null,null,null,null,null,null,"木製・外窓",16,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社日本の窓","W442W3232","MADOBA　ペア(Kr)","W2",null,null,null,null,null,null,"木製・外窓",16,null,null,null,"Low-E複層","クリプトンガス"]
["窓","株式会社日本の窓","W442B1213","MADOBA　防火窓","W3",null,null,null,null,null,null,"木製・外窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社日本の窓","W442B2223","MADOBA　防火窓(Ar)","W3",null,null,null,null,null,null,"木製・外窓",16,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社日本の窓","W442B3233","MADOBA　防火窓(Kr)","W3",null,null,null,null,null,null,"木製・外窓",16,null,null,null,"Low-E複層","クリプトンガス"]
["窓","株式会社日本の窓","W442W1213","MADOBA　ペア","W3",null,null,null,null,null,null,"木製・外窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社日本の窓","W447T7315","MADOBA　内窓トリプル","W5",null,null,null,null,null,null,"木製・内窓",12,12,null,null,"Low-E三層","乾燥空気"]
["窓","株式会社日本の窓","W447T8325","MADOBA　内窓トリプル(Ar)","W5",null,null,null,null,null,null,"木製・内窓",12,12,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社日本の窓","W447T9335","MADOBA　内窓トリプル(Kr)","W5",null,null,null,null,null,null,"木製・内窓",12,12,null,null,"Low-E三層","クリプトンガス"]
["窓","株式会社日本の窓","W447W7215","MADOBA　内窓","W5",null,null,null,null,null,null,"木製・内窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社日本の窓","W447W8225","MADOBA　内窓(Ar)","W5",null,null,null,null,null,null,"木製・内窓",16,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社日本の窓","W447W9235","MADOBA　内窓(Kr)","W5",null,null,null,null,null,null,"木製・内窓",16,null,null,null,"Low-E複層","クリプトンガス"]
["窓","株式会社日本産業","W371T1431","防犯ツインLow-Eトリプル樹脂サッシ","W1",null,null,null,null,null,null,"樹脂製・外窓",10,10,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社日本産業","W371T2431","防犯ツインLow-Eトリプル樹脂サッシ　テラスドア・勝手口ドア","W1",null,null,null,null,null,null,"樹脂製・外窓",10,10,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社日本産業","W371P1222","高性能樹脂サッシ","W2",null,null,null,null,null,null,"樹脂製・外窓",16,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社日本産業","W371P2222","高性能樹脂サッシ　テラスドア・勝手口ドア","W2",null,null,null,null,null,null,"樹脂製・外窓",16,null,null,null,"Low-E複層","アルゴンガス"]
["窓","日本ベルックス株式会社","W112E3322","GGU寒冷地 網入り透明複層 中軸回転式開閉型天窓","W2",null,null,null,null,null,null,"木製・外窓",12,12,null,null,"Low-E三層","アルゴンガス"]
["窓","日本ベルックス株式会社","W112E1224","FCMフィックス 型板網入り複層 フィックス型天窓","W4",null,null,null,null,null,null,"木製・外窓",8,null,null,null,"Low-E複層","アルゴンガス"]
["窓","日本ベルックス株式会社","W112E2224","FCMフィックス 透明合わせ複層 フィックス型天窓","W4",null,null,null,null,null,null,"木製・外窓",9,null,null,null,"Low-E複層","アルゴンガス"]
["窓","日本ベルックス株式会社","W112A1224","VS電動 透明合わせ複層　押し出し式開閉型天窓","W4",null,null,null,null,null,null,"木製・外窓",9,null,null,null,"Low-E複層","アルゴンガス"]
["窓","日本ベルックス株式会社","W112A2224","VS電動 網入り透明複層　押し出し式開閉型天窓","W4",null,null,null,null,null,null,"木製・外窓",8,null,null,null,"Low-E複層","アルゴンガス"]
["窓","日本ベルックス株式会社","W112A3224","VS電動 型板網入り複層　押し出し式開閉型天窓","W4",null,null,null,null,null,null,"木製・外窓",8,null,null,null,"Low-E複層","アルゴンガス"]
["窓","日本ベルックス株式会社","W112A4224","VS電動(白枠)網入り透明複層　押し出し式開閉型天窓","W4",null,null,null,null,null,null,"木製・外窓",8,null,null,null,"Low-E複層","アルゴンガス"]
["窓","日本ベルックス株式会社","W112B1224","VS手動 透明合わせ複層　押し出し式開閉型天窓","W4",null,null,null,null,null,null,"木製・外窓",9,null,null,null,"Low-E複層","アルゴンガス"]
["窓","日本ベルックス株式会社","W112B2224","VS手動 網入り透明複層　押し出し式開閉型天窓","W4",null,null,null,null,null,null,"木製・外窓",8,null,null,null,"Low-E複層","アルゴンガス"]
["窓","日本ベルックス株式会社","W112B3224","VS手動 型板網入り複層　押し出し式開閉型天窓","W4",null,null,null,null,null,null,"木製・外窓",8,null,null,null,"Low-E複層","アルゴンガス"]
["窓","日本ベルックス株式会社","W112B4224","VS手動(白枠)網入り透明複層　押し出し式開閉型天窓","W4",null,null,null,null,null,null,"木製・外窓",8,null,null,null,"Low-E複層","アルゴンガス"]
["窓","日本ベルックス株式会社","W112C1224","FSフィックス 透明合わせ複層　フィックス型天窓","W4",null,null,null,null,null,null,"木製・外窓",9,null,null,null,"Low-E複層","アルゴンガス"]
["窓","日本ベルックス株式会社","W112C2224","FSフィックス 網入り透明複層　フィックス型天窓","W4",null,null,null,null,null,null,"木製・外窓",8,null,null,null,"Low-E複層","アルゴンガス"]
["窓","日本ベルックス株式会社","W112C3224","FSフィックス 型板網入り複層　フィックス型天窓","W4",null,null,null,null,null,null,"木製・外窓",8,null,null,null,"Low-E複層","アルゴンガス"]
["窓","日本ベルックス株式会社","W112C4224","FSフィックス(白枠)網入り透明複層　フィックス型天窓","W4",null,null,null,null,null,null,"木製・外窓",8,null,null,null,"Low-E複層","アルゴンガス"]
["窓","日本ベルックス株式会社","W112D2224","GGL手動 網入り透明複層　中軸回転式開閉型天窓","W4",null,null,null,null,null,null,"木製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","日本ベルックス株式会社","W112E3224","GGL手動 透明合わせペア 3057","W4",null,null,null,null,null,null,"木製・外窓",15,null,null,null,"Low-E複層","アルゴンガス"]
["窓","フクビ化学工業株式会社","W356E1115","メルツェンサッシ　80型","W5",null,null,null,null,null,null,"樹脂製・内窓",12,null,null,null,"複層","乾燥空気"]
["窓","フクビ化学工業株式会社","W356E2215","メルツェンサッシ　80型 Low-E","W5",null,null,null,null,null,null,"樹脂製・内窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","フクビ化学工業株式会社","W356E3115","メルツェンサッシ　80型　テラスドア","W5",null,null,null,null,null,null,"樹脂製・内窓",12,null,null,null,"複層","乾燥空気"]
["窓","フクビ化学工業株式会社","W356E4215","メルツェンサッシ　80型　テラスドア Low-E","W5",null,null,null,null,null,null,"樹脂製・内窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","フクビ化学工業株式会社","W356S1115","メルツェンサッシ　66型","W5",null,null,null,null,null,null,"樹脂製・内窓",12,null,null,null,"複層","乾燥空気"]
["窓","フクビ化学工業株式会社","W356S2215","メルツェンサッシ　66型 Low-E","W5",null,null,null,null,null,null,"樹脂製・内窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","フクビ化学工業株式会社","W356S3115","メルツェンサッシ　66型　テラスドア","W5",null,null,null,null,null,null,"樹脂製・内窓",12,null,null,null,"複層","乾燥空気"]
["窓","フクビ化学工業株式会社","W356S4215","メルツェンサッシ　66型　テラスドア Low-E","W5",null,null,null,null,null,null,"樹脂製・内窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","フクビ化学工業株式会社","W356W1115","メルウィン","W5",null,null,null,null,null,null,"樹脂製・内窓",12,null,null,null,"複層","乾燥空気"]
["窓","フクビ化学工業株式会社","W356W2215","メルウィン Low-E","W5",null,null,null,null,null,null,"樹脂製・内窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","フクビ化学工業株式会社","W356W3115","メルウィン　テラスドア","W5",null,null,null,null,null,null,"樹脂製・内窓",12,null,null,null,"複層","乾燥空気"]
["窓","フクビ化学工業株式会社","W356W4215","メルウィン　テラスドア Low-E","W5",null,null,null,null,null,null,"樹脂製・内窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","不二サッシ株式会社","W033R1224","FNS-II100R","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","不二サッシ株式会社","W033R2214","FNS-II100R　框ドア","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","不二サッシ株式会社","W033S1341","FSSH　引違い(特定得意先向け用)","W1",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,0.2,null,null,"Low-E三層","真空"]
["窓","不二サッシ株式会社","W033S5341","FSSH　FIX(特定得意先向け用)","W1",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,0.2,null,null,"Low-E三層","真空"]
["窓","不二サッシ株式会社","W033S2342","FSSH　引違い(特定得意先向け用)","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,0.2,null,null,"Low-E三層","真空"]
["窓","不二サッシ株式会社","W033S6342","FSSH　FIX(特定得意先向け用)","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,0.2,null,null,"Low-E三層","真空"]
["窓","不二サッシ株式会社","W033S3322","FSSH　引違い(特定得意先向け用)","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",9,9,null,null,"Low-E三層","アルゴンガス"]
["窓","不二サッシ株式会社","W033S7322","FSSH　FIX(特定得意先向け用)","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",9,9,null,null,"Low-E三層","アルゴンガス"]
["窓","不二サッシ株式会社","W033S4223","FSSH　引違い(特定得意先向け用)","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","アルゴンガス"]
["窓","不二サッシ株式会社","W033S8223","FSSH　FIX(特定得意先向け用)","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","アルゴンガス"]
["窓","マーヴィンウィンドーズアンドドアーズ","W332W1222","マーヴィンアルティメットウッド","W2",null,null,null,null,null,null,"木製・外窓",11.5,null,null,null,"Low-E複層","アルゴンガス"]
["窓","マーヴィンウィンドーズアンドドアーズ","W331I1224","マーヴィンエレベイト","W4",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","マーヴィンウィンドーズアンドドアーズ","W334C1224","マーヴィンアルティメット","W4",null,null,null,null,null,null,"アルミ木複合製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W026A6115","インプラス for Renovation","W5",null,null,null,null,null,null,"樹脂製・内窓",8,null,null,null,"複層","乾燥空気"]
["窓","株式会社LIXIL","W026A7215","インプラス for Renovation Low-E","W5",null,null,null,null,null,null,"樹脂製・内窓",8,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W026A8225","インプラス for Renovation Low-E(Ar)","W5",null,null,null,null,null,null,"樹脂製・内窓",8,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W02FC3226","SAMOS-H RF(防火) Low-Eグリーン(Ar)","W6",null,null,null,null,null,null,"アルミ樹脂複合製・カバー(ビル用・防火仕様)",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023H5223","防火戸サーモスX シャッター付引違い窓 Low-E複層(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",15,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023S3214","サーモスII-H レール間カバー枠 Low-E W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W023S4224","サーモスII-H レール間カバー枠 Low-E(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W021E2431","エルスターX ダブルLow-E三層(Kr)W1","W1",null,null,null,null,null,null,"樹脂製・外窓",7,7,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W021L2431","エルスターX 勝手口ドア ダブルLow-E三層(Kr)W1","W1",null,null,null,null,null,null,"樹脂製・外窓",7,7,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W021L6431","エルスターX テラスドアTDF ダブルLow-E三層(Kr)W1","W1",null,null,null,null,null,null,"樹脂製・外窓",7,7,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W021L7431","エルスターX テラスドアTDFTD ダブルLow-E三層(Kr)W1","W1",null,null,null,null,null,null,"樹脂製・外窓",7,7,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W021L8431","エルスターX テラスドアTD ダブルLow-E三層(Kr)W1","W1",null,null,null,null,null,null,"樹脂製・外窓",7,7,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W021R1521","レガリスW1","W1",null,null,null,null,null,null,"樹脂製・外窓",14.5,13,13,14.5,"その他","アルゴンガス"]
["窓","株式会社LIXIL","W021R2521","レガリス テラスドアTDF W1","W1",null,null,null,null,null,null,"樹脂製・外窓",14.5,13,13,14.5,"その他","アルゴンガス"]
["窓","株式会社LIXIL","W021R3521","レガリス テラスドアTD W1","W1",null,null,null,null,null,null,"樹脂製・外窓",14.5,13,13,14.5,"その他","アルゴンガス"]
["窓","株式会社LIXIL","W021R4521","レガリス 勝手口ドアW1","W1",null,null,null,null,null,null,"樹脂製・外窓",14.5,13,13,14.5,"その他","アルゴンガス"]
["窓","株式会社LIXIL","W023F3431","サーモスX ダブルLow-E三層(Kr)W1","W1",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",8,9,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W023F5421","LW ダブルLow-E三層(Ar)W1","W1",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",11,12,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023F5431","LW ダブルLow-E三層(Kr)W1","W1",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",6,7,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W023H3431","防火戸サーモスX シャッター付引違い窓 ダブルLow-E三層(Kr)W1","W1",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",10,10,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W023M7431","サーモスX テラスドア ダブルLow-E三層(Kr)W1","W1",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",8,9,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W023M8431","サーモスX 採風勝手口ドア ダブルLow-E三層(Kr)W1","W1",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",8,9,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W023M9431","サーモスX 勝手口ドア ダブルLow-E三層(Kr)W1","W1",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",8,9,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W021E1322","エルスターX Low-E三層(Ar)W2","W2",null,null,null,null,null,null,"樹脂製・外窓",11,11,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021E1332","エルスターX Low-E三層(Kr)W2","W2",null,null,null,null,null,null,"樹脂製・外窓",7,7,null,null,"Low-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W021E2422","エルスターX ダブルLow-E三層(Ar)W2","W2",null,null,null,null,null,null,"樹脂製・外窓",7,7,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021E2432","エルスターX ダブルLow-E三層(Kr)W2","W2",null,null,null,null,null,null,"樹脂製・外窓",6,6,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W021L1322","エルスターX 勝手口ドア Low-E三層(Ar)W2","W2",null,null,null,null,null,null,"樹脂製・外窓",11,11,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021L1332","エルスターX 勝手口ドア Low-E三層(Kr)W2","W2",null,null,null,null,null,null,"樹脂製・外窓",7,7,null,null,"Low-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W021L2422","エルスターX 勝手口ドア ダブルLow-E三層(Ar)W2","W2",null,null,null,null,null,null,"樹脂製・外窓",7,7,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021L2432","エルスターX 勝手口ドア ダブルLow-E三層(Kr)W2","W2",null,null,null,null,null,null,"樹脂製・外窓",6,6,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W021L3322","エルスターX テラスドアTDF Low-E三層(Ar)W2","W2",null,null,null,null,null,null,"樹脂製・外窓",11,11,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021L3332","エルスターX テラスドアTDF Low-E三層(Kr)W2","W2",null,null,null,null,null,null,"樹脂製・外窓",7,7,null,null,"Low-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W021L4322","エルスターX テラスドアTDFTD Low-E三層(Ar)W2","W2",null,null,null,null,null,null,"樹脂製・外窓",11,11,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021L4332","エルスターX テラスドアTDFTD Low-E三層(Kr)W2","W2",null,null,null,null,null,null,"樹脂製・外窓",7,7,null,null,"Low-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W021L5322","エルスターX テラスドアTD Low-E三層(Ar)W2","W2",null,null,null,null,null,null,"樹脂製・外窓",11,11,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021L5332","エルスターX テラスドアTD Low-E三層(Kr)W2","W2",null,null,null,null,null,null,"樹脂製・外窓",7,7,null,null,"Low-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W021L6422","エルスターX テラスドアTDF ダブルLow-E三層(Ar)W2","W2",null,null,null,null,null,null,"樹脂製・外窓",7,7,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021L6432","エルスターX テラスドアTDF ダブルLow-E三層(Kr)W2","W2",null,null,null,null,null,null,"樹脂製・外窓",6,6,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W021L7422","エルスターX テラスドアTDFTD ダブルLow-E三層(Ar)W2","W2",null,null,null,null,null,null,"樹脂製・外窓",7,7,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021L7432","エルスターX テラスドアTDFTD ダブルLow-E三層(Kr)W2","W2",null,null,null,null,null,null,"樹脂製・外窓",6,6,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W021L8422","エルスターX テラスドアTD ダブルLow-E三層(Ar)W2","W2",null,null,null,null,null,null,"樹脂製・外窓",7,7,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021L8432","エルスターX テラスドアTD ダブルLow-E三層(Kr)W2","W2",null,null,null,null,null,null,"樹脂製・外窓",6,6,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W023F2332","サーモスX Low-E三層(Kr)W2","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",7,8,null,null,"Low-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W023F3422","サーモスX ダブルLow-E三層(Ar)W2","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",7,8,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023F3432","サーモスX ダブルLow-E三層(Kr)W2","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",6,6,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W023F5422","LW ダブルLow-E三層(Ar)W2","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",6,7,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023F6322","LW Low-E三層(Ar)W2","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",10,11,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023F6332","LW Low-E三層(Kr)W2","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",6,7,null,null,"Low-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W023H2332","防火戸サーモスX シャッター付引違い窓 Low-E三層(Kr)W2","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",7,8,null,null,"Low-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W023H3422","防火戸サーモスX シャッター付引違い窓 ダブルLow-E三層(Ar)W2","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",8,9,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023H3432","防火戸サーモスX シャッター付引違い窓 ダブルLow-E三層(Kr)W2","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",6,6,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W023M4332","サーモスX テラスドア Low-E三層(Kr)W2","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",7,8,null,null,"Low-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W023M5332","サーモスX 採風勝手口ドア Low-E三層(Kr)W2","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",7,8,null,null,"Low-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W023M6332","サーモスX 勝手口ドア Low-E三層(Kr)W2","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",7,8,null,null,"Low-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W023M7422","サーモスX テラスドア ダブルLow-E三層(Ar)W2","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",7,8,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023M7432","サーモスX テラスドア ダブルLow-E三層(Kr)W2","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",6,6,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W023M8422","サーモスX 採風勝手口ドア ダブルLow-E三層(Ar)W2","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",7,8,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023M8432","サーモスX 採風勝手口ドア ダブルLow-E三層(Kr)W2","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",6,6,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W023M9422","サーモスX 勝手口ドア ダブルLow-E三層(Ar)W2","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",7,8,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023M9432","サーモスX 勝手口ドア ダブルLow-E三層(Kr)W2","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",6,6,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W021D1213","エルスターS Low-E W3","W3",null,null,null,null,null,null,"樹脂製・外窓",14,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W021D2223","エルスターS Low-E(Ar)W3","W3",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W021E1323","エルスターX Low-E三層(Ar)W3","W3",null,null,null,null,null,null,"樹脂製・外窓",7,7,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021E2423","エルスターX ダブルLow-E三層(Ar)W3","W3",null,null,null,null,null,null,"樹脂製・外窓",6,6,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021K1213","エルスターS テラスドアTDF Low-E W3","W3",null,null,null,null,null,null,"樹脂製・外窓",14,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W021K2213","エルスターS テラスドアTDFTD Low-E W3","W3",null,null,null,null,null,null,"樹脂製・外窓",14,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W021K3213","エルスターS テラスドアTD Low-E W3","W3",null,null,null,null,null,null,"樹脂製・外窓",14,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W021K4213","エルスターS 勝手口ドア Low-E W3","W3",null,null,null,null,null,null,"樹脂製・外窓",14,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W021K5223","エルスターS テラスドアTDF Low-E(Ar)W3","W3",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W021K6223","エルスターS テラスドアTDFTD Low-E(Ar)W3","W3",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W021K7223","エルスターS テラスドアTD Low-E(Ar)W3","W3",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W021K8223","エルスターS 勝手口ドア Low-E(Ar)W3","W3",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W021L1323","エルスターX 勝手口ドア Low-E三層(Ar)W3","W3",null,null,null,null,null,null,"樹脂製・外窓",7,7,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021L2423","エルスターX 勝手口ドア ダブルLow-E三層(Ar)W3","W3",null,null,null,null,null,null,"樹脂製・外窓",6,6,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021L3323","エルスターX テラスドアTDF Low-E三層(Ar)W3","W3",null,null,null,null,null,null,"樹脂製・外窓",7,7,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021L4323","エルスターX テラスドアTDFTD Low-E三層(Ar)W3","W3",null,null,null,null,null,null,"樹脂製・外窓",7,7,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021L5323","エルスターX テラスドアTD Low-E三層(Ar)W3","W3",null,null,null,null,null,null,"樹脂製・外窓",7,7,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021L6423","エルスターX テラスドアTDF ダブルLow-E三層(Ar)W3","W3",null,null,null,null,null,null,"樹脂製・外窓",6,6,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021L7423","エルスターX テラスドアTDFTD ダブルLow-E三層(Ar)W3","W3",null,null,null,null,null,null,"樹脂製・外窓",6,6,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021L8423","エルスターX テラスドアTD ダブルLow-E三層(Ar)W3","W3",null,null,null,null,null,null,"樹脂製・外窓",6,6,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023F1223","サーモスX Low-E複層(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",15,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023F2323","サーモスX Low-E三層(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",7,8,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023F2333","サーモスX Low-E三層(Kr)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",4,5,null,null,"Low-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W023F3423","サーモスX ダブルLow-E三層(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",6,6,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023F6323","LW Low-E三層(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",6,7,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023F7223","LW Low-E複層(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",15,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023H2323","防火戸サーモスX シャッター付引違い窓 Low-E三層(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",7,8,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023H2333","防火戸サーモスX シャッター付引違い窓 Low-E三層(Kr)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",4,5,null,null,"Low-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W023H3423","防火戸サーモスX シャッター付引違い窓 ダブルLow-E三層(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",6,6,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023M1223","サーモスX テラスドア Low-E複層(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",15,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023M2223","サーモスX 採風勝手口ドア Low-E複層(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",15,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023M3223","サーモスX 勝手口ドア Low-E複層(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",15,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023M4323","サーモスX テラスドア Low-E三層(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",7,8,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023M4333","サーモスX テラスドア Low-E三層(Kr)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",4,5,null,null,"Low-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W023M5323","サーモスX 採風勝手口ドア Low-E三層(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",7,8,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023M5333","サーモスX 採風勝手口ドア Low-E三層(Kr)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",4,5,null,null,"Low-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W023M6323","サーモスX 勝手口ドア Low-E三層(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",7,8,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023M6333","サーモスX 勝手口ドア Low-E三層(Kr)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",4,5,null,null,"Low-E三層","クリプトンガス"]
["窓","株式会社LIXIL","W023M7423","サーモスX テラスドア ダブルLow-E三層(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",6,6,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023M8423","サーモスX 採風勝手口ドア ダブルLow-E三層(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",6,6,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023M9423","サーモスX 勝手口ドア ダブルLow-E三層(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",6,6,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023Z2223","PRESEA-H Low-Eグリーン(Ar)W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W021D1214","エルスターS Low-E W4","W4",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W021E1324","エルスターX Low-E三層(Ar)W4","W4",null,null,null,null,null,null,"樹脂製・外窓",4,5,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021K1214","エルスターS テラスドアTDF Low-E W4","W4",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W021K2214","エルスターS テラスドアTDFTD Low-E W4","W4",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W021K3214","エルスターS テラスドアTD Low-E W4","W4",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W021K4214","エルスターS 勝手口ドア Low-E W4","W4",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W021L1324","エルスターX 勝手口ドア Low-E三層(Ar)W4","W4",null,null,null,null,null,null,"樹脂製・外窓",4,5,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021L3324","エルスターX テラスドアTDF Low-E三層(Ar)W4","W4",null,null,null,null,null,null,"樹脂製・外窓",4,5,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021L4324","エルスターX テラスドアTDFTD Low-E三層(Ar)W4","W4",null,null,null,null,null,null,"樹脂製・外窓",4,5,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W021L5324","エルスターX テラスドアTD Low-E三層(Ar)W4","W4",null,null,null,null,null,null,"樹脂製・外窓",4,5,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023F2324","サーモスX Low-E三層(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",4,5,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023F8214","LW Low-E複層 W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",15,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W023G4224","防火戸FG-F Low-E(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023H1224","防火戸サーモスX Low-E複層(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",15,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023H2324","防火戸サーモスX シャッター付引違い窓 Low-E三層(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",4,5,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023H4224","防火戸サーモスX 採風勝手口ドア Low-E複層(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",15,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023M4324","サーモスX テラスドア Low-E三層(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",4,5,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023M5324","サーモスX 採風勝手口ドア Low-E三層(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",4,5,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023M6324","サーモスX 勝手口ドア Low-E三層(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",4,5,null,null,"Low-E三層","アルゴンガス"]
["窓","株式会社LIXIL","W023S1214","サーモスII-H Low-E W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",14,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W023S2224","サーモスII-H Low-E(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",10,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023T1214","サーモスII-H テラスドア Low-E W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",14,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W023T3214","サーモスII-H 勝手口ドア 全面ガラス Low-E W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",14,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W023T5224","サーモスII-H テラスドア Low-E(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",10,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023T7224","サーモスII-H 勝手口ドア 全面ガラス Low-E(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",10,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023U1214","サーモスL Low-E W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W023U2224","サーモスL Low-E(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023V1214","サーモスL テラスドア Low-E W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W023V3214","サーモスL 勝手口ドア 全面ガラス Low-E W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W023V5224","サーモスL テラスドア Low-E(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023V7224","サーモスL 勝手口ドア 全面ガラス Low-E(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023W1214","サーモスL 高断熱枠 Low-E W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",14,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W023W2224","サーモスL 高断熱枠 Low-E(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",10,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023X1214","シンフォニーウッディ/マイルド Low-E W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",15,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W023X2214","シンフォニーウッディ/マイルド テラスドア Low-E W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",15,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W023X5224","シンフォニーウッディ/マイルド Low-E(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023X6224","シンフォニーウッディ/マイルド テラスドア Low-E(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023Y1224","防火戸FG-H シャッター付引違い窓 Low-E(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023Y2224","防火戸FG-C シャッター付引違い窓 Low-E(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023Y3224","防火戸FG-H Low-E(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023Y5224","防火戸FG-L Low-E(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023Y7224","防火戸FG-L シャッター付引違い窓 Low-E(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",13,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W023Z1214","PRESEA-H(防火) Low-EグリーンW4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",10,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W023Z3214","PRESEA-H かまちドア Low-EグリーンW4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W02BP2224","リプラス 専用枠 Low-E(Ar)W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・カバー(住宅用)",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W026A1115","インプラス 一般複層","W5",null,null,null,null,null,null,"樹脂製・内窓",8,null,null,null,"複層","乾燥空気"]
["窓","株式会社LIXIL","W026A2215","インプラス Low-E","W5",null,null,null,null,null,null,"樹脂製・内窓",8,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W026A3225","インプラス Low-E(Ar)","W5",null,null,null,null,null,null,"樹脂製・内窓",8,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W026A4245","インプラス 真空ガラス","W5",null,null,null,null,null,null,"樹脂製・内窓",0.2,null,null,null,"Low-E複層","真空"]
["窓","株式会社LIXIL","W026A5145","インプラス 真空ガラス(一般)","W5",null,null,null,null,null,null,"樹脂製・内窓",0.2,null,null,null,"複層","真空"]
["窓","株式会社LIXIL","W026B1115","インプラスウッド 一般複層","W5",null,null,null,null,null,null,"樹脂製・内窓",8,null,null,null,"複層","乾燥空気"]
["窓","株式会社LIXIL","W026B2215","インプラスウッド Low-E","W5",null,null,null,null,null,null,"樹脂製・内窓",8,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W026B3225","インプラスウッド Low-E(Ar)","W5",null,null,null,null,null,null,"樹脂製・内窓",8,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W026B4245","インプラスウッド 真空ガラス","W5",null,null,null,null,null,null,"樹脂製・内窓",0.2,null,null,null,"Low-E複層","真空"]
["窓","株式会社LIXIL","W026B5145","インプラスウッド 真空ガラス(一般)","W5",null,null,null,null,null,null,"樹脂製・内窓",0.2,null,null,null,"複層","真空"]
["窓","株式会社LIXIL","W026J1115","インプラステラスドア 一般複層","W5",null,null,null,null,null,null,"樹脂製・内窓",8,null,null,null,"複層","乾燥空気"]
["窓","株式会社LIXIL","W026J2215","インプラステラスドア Low-E","W5",null,null,null,null,null,null,"樹脂製・内窓",8,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社LIXIL","W026J3225","インプラステラスドア Low-E(Ar)","W5",null,null,null,null,null,null,"樹脂製・内窓",8,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W026J4245","インプラステラスドア 真空ガラス","W5",null,null,null,null,null,null,"樹脂製・内窓",0.2,null,null,null,"Low-E複層","真空"]
["窓","株式会社LIXIL","W026J5145","インプラス テラスドア 真空ガラス(一般)","W5",null,null,null,null,null,null,"樹脂製・内窓",0.2,null,null,null,"複層","真空"]
["窓","株式会社LIXIL","W02DG6226","SAMOS-H RF Low-Eグリーン(Ar)","W6",null,null,null,null,null,null,"アルミ樹脂複合製・カバー(ビル用)",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社LIXIL","W02FC2216","SAMOS-H RF(防火) Low-Eグリーン","W6",null,null,null,null,null,null,"アルミ樹脂複合製・カバー(ビル用・防火仕様)",10,null,null,null,"Low-E複層","乾燥空気"]
["窓","株式会社菱晃","W453G1223","高断熱ｶﾞﾗｽﾌﾗｯﾄGFD　LOW-E(Ar)","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","株式会社菱晃","W453G2114","高断熱ｶﾞﾗｽﾌﾗｯﾄGFD","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",12,null,null,null,"複層","乾燥空気"]
["窓","株式会社菱晃","W453G3224","高断熱ｶﾞﾗｽﾌﾗｯﾄGFDL　LOW-E(Ar)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W04DZ3226","エピソードNEO-LB[GRAF工法]樹脂スペーサー","W6",null,null,null,null,null,null,"アルミ樹脂複合製・カバー(ビル用)",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041N2421","APW430防火窓 (日射遮蔽型)(Ar)　W1","W1",null,null,null,null,null,null,"樹脂製・外窓",11,11,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041N4421","APW431防火窓 (日射遮蔽型)(Ar)　W1","W1",null,null,null,null,null,null,"樹脂製・外窓",12,12,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041S4431","APW431+ (日射遮蔽型)(Kr)　W1","W1",null,null,null,null,null,null,"樹脂製・外窓",10,10,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","YKK AP株式会社","W041A1322","APW430 (日射取得型)(Ar)　W2","W2",null,null,null,null,null,null,"樹脂製・外窓",10,10,null,null,"Low-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041A2422","APW430 (日射遮蔽型)(Ar)　W2","W2",null,null,null,null,null,null,"樹脂製・外窓",10,10,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041B2422","APW431 (日射遮蔽型)(Ar)　W2","W2",null,null,null,null,null,null,"樹脂製・外窓",10,10,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041N1322","APW430防火窓 (日射取得型)(Ar)　W2","W2",null,null,null,null,null,null,"樹脂製・外窓",10,10,null,null,"Low-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041N2422","APW430防火窓 (日射遮蔽型)(Ar)　W2","W2",null,null,null,null,null,null,"樹脂製・外窓",10,10,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041N3322","APW431防火窓 (日射取得型)(Ar)　W2","W2",null,null,null,null,null,null,"樹脂製・外窓",10,10,null,null,"Low-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041N4422","APW431防火窓 (日射遮蔽型)(Ar)　W2","W2",null,null,null,null,null,null,"樹脂製・外窓",10,10,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041U6442","APW330防火窓　木目仕様(真空トリプル) W2","W2",null,null,null,null,null,null,"樹脂製・外窓",12,0.2,null,null,"ダブルLow-E三層","真空"]
["窓","YKK AP株式会社","W041U7442","APW331防火窓　木目仕様(真空トリプル) W2","W2",null,null,null,null,null,null,"樹脂製・外窓",12,0.2,null,null,"ダブルLow-E三層","真空"]
["窓","YKK AP株式会社","W043P1422","APW511　トリプルガラス W2","W2",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",10,10,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041U6223","APW330防火窓　木目仕様(Ar) W3","W3",null,null,null,null,null,null,"樹脂製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041U7223","APW331防火窓　木目仕様(Ar) W3","W3",null,null,null,null,null,null,"樹脂製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W043P1423","APW511　トリプルガラス W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",8,8,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W043P2223","APW511　Low-E複層ガラス(日射取得型)(Ar・樹脂SP) W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W043P3223","APW511　Low-E複層ガラス(日射遮蔽型)(Ar) W3","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041U6214","APW330防火窓　木目仕様 W4","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041U6224","APW330防火窓　木目仕様(Ar) W4","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041U7214","APW331防火窓　木目仕様 W4","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041U7224","APW331防火窓　木目仕様(Ar) W4","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041U8214","APW331防火窓　木目仕様開き窓テラス(2シリンダー仕様) W4","W4",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041U8224","APW331防火窓　木目仕様開き窓テラス(2シリンダー仕様)(Ar) W4","W4",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W043M4224","エピソードNEO-R (Ar・樹脂SP) W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W043P2214","APW511　Low-E複層ガラス(日射取得型) W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",14,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W043P2224","APW511　Low-E複層ガラス(日射取得型)(Ar) W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W043P3214","APW511　Low-E複層ガラス(日射遮蔽型) W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",14,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041A1321","APW430 (日射取得型)","W1",null,null,null,null,null,null,"樹脂製・外窓",12,12,null,null,"Low-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041A2421","APW430 (日射遮蔽型)","W1",null,null,null,null,null,null,"樹脂製・外窓",11,11,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041B2421","APW431 (日射遮蔽型)","W1",null,null,null,null,null,null,"樹脂製・外窓",11,11,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041B4421","APW431 ﾃﾗｽﾄﾞｱ+FIX連窓(日射遮蔽型)","W1",null,null,null,null,null,null,"樹脂製・外窓",14,14,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041B5321","APW431 ﾃﾗｽﾄﾞｱ+FIX連窓(日射取得型)","W1",null,null,null,null,null,null,"樹脂製・外窓",16,16,null,null,"Low-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041B7421","APW431 ﾃﾗｽﾄﾞｱ(日射遮蔽型)","W1",null,null,null,null,null,null,"樹脂製・外窓",14,14,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041B8421","APW431 勝手口ﾄﾞｱ中桟無","W1",null,null,null,null,null,null,"樹脂製・外窓",14,14,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041E2441","APW330 (真空ﾄﾘﾌﾟﾙ)","W1",null,null,null,null,null,null,"樹脂製・外窓",12,0.2,null,null,"ダブルLow-E三層","真空"]
["窓","YKK AP株式会社","W041F5441","APW331 ﾃﾗｽﾄﾞｱ(真空ﾄﾘﾌﾟﾙ)","W1",null,null,null,null,null,null,"樹脂製・外窓",12,0.2,null,null,"ダブルLow-E三層","真空"]
["窓","YKK AP株式会社","W041R1431","APW430+ (Kr)(日射遮蔽型)","W1",null,null,null,null,null,null,"樹脂製・外窓",10,10,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","YKK AP株式会社","W041R2421","APW430+ (Ar)(日射遮蔽型)","W1",null,null,null,null,null,null,"樹脂製・外窓",14,14,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041R3321","APW430+ (Ar)(日射取得型)","W1",null,null,null,null,null,null,"樹脂製・外窓",14,14,null,null,"Low-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041R4431","APW431+ (Kr)ﾃﾗｽﾄﾞｱ+FIX連窓(日射遮蔽型)","W1",null,null,null,null,null,null,"樹脂製・外窓",14,14,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","YKK AP株式会社","W041R5421","APW431+ (Ar)ﾃﾗｽﾄﾞｱ+FIX連窓(日射遮蔽型)","W1",null,null,null,null,null,null,"樹脂製・外窓",14,14,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041R6321","APW431+ (Ar)ﾃﾗｽﾄﾞｱ+FIX連窓(日射取得型)","W1",null,null,null,null,null,null,"樹脂製・外窓",14,14,null,null,"Low-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041R7431","APW431+ (Kr)ﾃﾗｽﾄﾞｱ(日射遮蔽型)","W1",null,null,null,null,null,null,"樹脂製・外窓",14,14,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","YKK AP株式会社","W041R8421","APW431+ (Ar)ﾃﾗｽﾄﾞｱ(日射遮蔽型)","W1",null,null,null,null,null,null,"樹脂製・外窓",14,14,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041R9321","APW431+ (Ar)ﾃﾗｽﾄﾞｱ(日射取得型)","W1",null,null,null,null,null,null,"樹脂製・外窓",14,14,null,null,"Low-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041S1431","APW431+ (Kr)勝手口ﾄﾞｱ中桟無(日射遮蔽型)","W1",null,null,null,null,null,null,"樹脂製・外窓",14,14,null,null,"ダブルLow-E三層","クリプトンガス"]
["窓","YKK AP株式会社","W041S2421","APW431+ (Ar)勝手口ﾄﾞｱ中桟無(日射遮蔽型)","W1",null,null,null,null,null,null,"樹脂製・外窓",14,14,null,null,"ダブルLow-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041T5441","APW331 木目仕様ﾃﾗｽﾄﾞｱ(真空ﾄﾘﾌﾟﾙ)","W1",null,null,null,null,null,null,"樹脂製・外窓",12,0.2,null,null,"ダブルLow-E三層","真空"]
["窓","YKK AP株式会社","W041B1322","APW431 (日射取得型)","W2",null,null,null,null,null,null,"樹脂製・外窓",10,10,null,null,"Low-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041B3322","APW431 ﾃﾗｽﾄﾞｱ+FIX連窓(日射取得型)","W2",null,null,null,null,null,null,"樹脂製・外窓",14,14,null,null,"Low-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041B6322","APW431 ﾃﾗｽﾄﾞｱ(日射取得型)","W2",null,null,null,null,null,null,"樹脂製・外窓",14,14,null,null,"Low-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041B9322","APW431 勝手口ﾄﾞｱ中桟無(日射取得型)","W2",null,null,null,null,null,null,"樹脂製・外窓",14,14,null,null,"Low-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041C7222","APW330 (Ar)","W2",null,null,null,null,null,null,"樹脂製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041C8212","APW330 ﾂｰｱｸｼｮﾝ窓(日射遮蔽型)","W2",null,null,null,null,null,null,"樹脂製・外窓",15,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041C9222","APW330 ﾂｰｱｸｼｮﾝ窓(Ar)","W2",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041D9222","APW331 (日射遮蔽型)(Ar)","W2",null,null,null,null,null,null,"樹脂製・外窓",15,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041E5222","APW330 木目仕様(日射遮蔽型)(Ar)","W2",null,null,null,null,null,null,"樹脂製・外窓",15,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041E6442","APW330 木目仕様(真空ﾄﾘﾌﾟﾙ)","W2",null,null,null,null,null,null,"樹脂製・外窓",12,0.2,null,null,"ダブルLow-E三層","真空"]
["窓","YKK AP株式会社","W041F3222","APW331 ﾃﾗｽﾄﾞｱ(日射遮蔽型)(Ar)","W2",null,null,null,null,null,null,"樹脂製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041F4442","APW331 (真空ﾄﾘﾌﾟﾙ)","W2",null,null,null,null,null,null,"樹脂製・外窓",12,0.2,null,null,"ダブルLow-E三層","真空"]
["窓","YKK AP株式会社","W041F6442","APW331 勝手口ﾄﾞｱ中桟無(真空ﾄﾘﾌﾟﾙ)","W2",null,null,null,null,null,null,"樹脂製・外窓",12,0.2,null,null,"ダブルLow-E三層","真空"]
["窓","YKK AP株式会社","W041F9222","APW331 勝手口ﾄﾞｱ中桟無(日射遮蔽型)(Ar)","W2",null,null,null,null,null,null,"樹脂製・外窓",15,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041G4222","APW330防火窓 (Ar)","W2",null,null,null,null,null,null,"樹脂製・外窓",13,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041J5222","ﾌﾟﾗﾏｰﾄﾞH (日射遮蔽型)(Ar)(樹脂ｽﾍﾟｰｻｰ) W2","W2",null,null,null,null,null,null,"樹脂製・外窓",13,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041K9222","ﾌﾟﾗﾏｰﾄﾞIII ﾃﾗｽﾄﾞｱ+FIX連窓(日射遮蔽型)(Ar)","W2",null,null,null,null,null,null,"樹脂製・外窓",15,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041S3322","APW431+ (Ar)勝手口ドア中桟無(日射取得型)","W2",null,null,null,null,null,null,"樹脂製・外窓",14,14,null,null,"Low-E三層","アルゴンガス"]
["窓","YKK AP株式会社","W041T1442","APW331 木目仕様(真空ﾄﾘﾌﾟﾙ)","W2",null,null,null,null,null,null,"樹脂製・外窓",12,0.2,null,null,"ダブルLow-E三層","真空"]
["窓","YKK AP株式会社","W041T9442","APW331 木目仕様勝手口ﾄﾞｱ中桟無(真空ﾄﾘﾌﾟﾙ)","W2",null,null,null,null,null,null,"樹脂製・外窓",12,0.2,null,null,"ダブルLow-E三層","真空"]
["窓","YKK AP株式会社","W041U1222","APW331防火窓 開き窓ﾃﾗｽ 2ｼﾘﾝﾀﾞｰ仕様 (日射遮蔽型)(Ar)","W2",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041U3222","APW331防火窓 開き窓ﾃﾗｽ 2ｼﾘﾝﾀﾞｰ仕様 (日射取得型)(Ar)","W2",null,null,null,null,null,null,"樹脂製・外窓",13,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041C3213","APW330 ﾂｰｱｸｼｮﾝ窓","W3",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041C5213","APW330","W3",null,null,null,null,null,null,"樹脂製・外窓",15,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041C6223","APW330 (Ar)","W3",null,null,null,null,null,null,"樹脂製・外窓",13,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041D7213","APW331 (日射遮蔽型)","W3",null,null,null,null,null,null,"樹脂製・外窓",15,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041D8223","APW331 (Ar)","W3",null,null,null,null,null,null,"樹脂製・外窓",13,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041E3213","APW330 木目仕様(日射遮蔽型)","W3",null,null,null,null,null,null,"樹脂製・外窓",15,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041E5223","APW330 木目仕様(Ar)","W3",null,null,null,null,null,null,"樹脂製・外窓",13,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041E9223","APW331 木目仕様(Ar)","W3",null,null,null,null,null,null,"樹脂製・外窓",13,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041F1213","APW331 ﾃﾗｽﾄﾞｱ","W3",null,null,null,null,null,null,"樹脂製・外窓",15,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041F2223","APW331 ﾃﾗｽﾄﾞｱ(Ar)","W3",null,null,null,null,null,null,"樹脂製・外窓",13,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041F7213","APW331 勝手口ﾄﾞｱ中桟無(日射遮蔽型)","W3",null,null,null,null,null,null,"樹脂製・外窓",15,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041F8223","APW331 勝手口ﾄﾞｱ中桟無(Ar)","W3",null,null,null,null,null,null,"樹脂製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041G3223","APW330防火窓 (日射遮蔽型)(Ar)","W3",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041H5223","APW331防火窓 引違い窓ﾃﾗｽ戸(日射遮蔽型)(Ar)","W3",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041H7223","APW331防火窓 引違い窓ﾃﾗｽ戸(日射取得型)(Ar)","W3",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041J3223","ﾌﾟﾗﾏｰﾄﾞIII (Ar)","W3",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041J4213","ﾌﾟﾗﾏｰﾄﾞIII (日射遮蔽型)","W3",null,null,null,null,null,null,"樹脂製・外窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041J6223","ﾌﾟﾗﾏｰﾄﾞH (Ar) W3","W3",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041J7223","ﾌﾟﾗﾏｰﾄﾞH ﾃﾗｽﾄﾞｱ(Ar) W3","W3",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041J8223","ﾌﾟﾗﾏｰﾄﾞH ﾃﾗｽﾄﾞｱ+FIX連窓(Ar) W3","W3",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041K8223","ﾌﾟﾗﾏｰﾄﾞIII ﾃﾗｽﾄﾞｱ+FIX連窓(Ar)","W3",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041T4223","APW331 木目仕様ﾃﾗｽﾄﾞｱ(Ar)","W3",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041T8223","APW331 木目仕様勝手口ﾄﾞｱ中桟無(Ar)","W3",null,null,null,null,null,null,"樹脂製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041U2223","APW331防火窓 開き窓ﾃﾗｽ 2ｼﾘﾝﾀﾞｰ仕様 (日射取得型)(Ar)","W3",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041U4213","APW331防火窓 開き窓ﾃﾗｽ 2ｼﾘﾝﾀﾞｰ仕様 (日射遮蔽型)","W3",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041U5213","APW331防火窓 開き窓ﾃﾗｽ 2ｼﾘﾝﾀﾞｰ仕様 (日射取得型)","W3",null,null,null,null,null,null,"樹脂製・外窓",13,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041V1213","ﾌﾟﾗﾏｰﾄﾞIII ﾃﾗｽﾄﾞｱ+FIX連窓","W3",null,null,null,null,null,null,"樹脂製・外窓",14,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041V2223","ﾌﾟﾗﾏｰﾄﾞIII ﾃﾗｽﾄﾞｱ(Ar)","W3",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041V3213","ﾌﾟﾗﾏｰﾄﾞIII ﾃﾗｽﾄﾞｱ(日射遮蔽型)","W3",null,null,null,null,null,null,"樹脂製・外窓",15,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041V4223","ﾌﾟﾗﾏｰﾄﾞH 片開きﾄﾞｱ(断熱腰ﾊﾟﾈﾙ仕様除く)(Ar) W3","W3",null,null,null,null,null,null,"樹脂製・外窓",15,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041Y1213","ﾌﾟﾗﾏｰﾄﾞH 遮熱ﾌﾞﾙｰ W3","W3",null,null,null,null,null,null,"樹脂製・外窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041Y2223","ﾌﾟﾗﾏｰﾄﾞH (Ar) W3","W3",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041Y4213","ﾌﾟﾗﾏｰﾄﾞH ﾃﾗｽﾄﾞｱ(断熱腰ﾊﾟﾈﾙ仕様除く) W3","W3",null,null,null,null,null,null,"樹脂製・外窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041Y5223","ﾌﾟﾗﾏｰﾄﾞH (Ar)ﾃﾗｽﾄﾞｱ(断熱腰ﾊﾟﾈﾙ仕様除く) W3","W3",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W043L4223","ｴﾋﾟｿｰﾄﾞNEO (日射遮蔽型)(Ar)","W3",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W04AW0223","ﾏﾄﾞﾘﾓ 樹脂窓 北海道(Ar) W3","W3",null,null,null,null,null,null,"樹脂製・カバー(住宅用)",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W04AW2213","ﾏﾄﾞﾘﾓ 樹脂窓 北海道樹脂ｽﾍﾟｰｻｰ W3","W3",null,null,null,null,null,null,"樹脂製・カバー(住宅用)",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W04AW4223","ﾏﾄﾞﾘﾓ 樹脂窓 北海道(Ar)片開きﾄﾞｱ 全面ｶﾞﾗｽﾀｲﾌﾟ W3","W3",null,null,null,null,null,null,"樹脂製・カバー(住宅用)",13,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W04AX0223","ﾏﾄﾞﾘﾓ 断熱窓 樹脂窓(Ar) W3","W3",null,null,null,null,null,null,"樹脂製・カバー(住宅用)",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W04AX2213","ﾏﾄﾞﾘﾓ 断熱窓 樹脂窓 W3","W3",null,null,null,null,null,null,"樹脂製・カバー(住宅用)",14,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041C1214","APW330","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041C2224","APW330 (Ar)","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041D1214","APW331","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041D2224","APW331 (Ar)","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041D3214","APW331 ﾃﾗｽﾄﾞｱ","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041D4214","APW331 勝手口ﾄﾞｱ中桟無","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041D5224","APW331 ﾃﾗｽﾄﾞｱ(Ar)","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041D6224","APW331 勝手口ﾄﾞｱ中桟無(Ar)","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041E3214","APW330 木目仕様","W4",null,null,null,null,null,null,"樹脂製・外窓",10,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041E4224","APW330 木目仕様(Ar)","W4",null,null,null,null,null,null,"樹脂製・外窓",10,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041E7214","APW331 木目仕様","W4",null,null,null,null,null,null,"樹脂製・外窓",10,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041E8224","APW331 木目仕様(Ar)","W4",null,null,null,null,null,null,"樹脂製・外窓",10,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041G1214","APW330防火窓","W4",null,null,null,null,null,null,"樹脂製・外窓",10,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041G2224","APW330防火窓 (Ar)","W4",null,null,null,null,null,null,"樹脂製・外窓",10,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041H1214","APW331防火窓","W4",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041H2224","APW331防火窓 (Ar)","W4",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041H3214","APW331防火窓 開き窓ﾃﾗｽ 2ｼﾘﾝﾀﾞｰ仕様","W4",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041H6224","APW331防火窓 引違い窓ﾃﾗｽ戸(日射取得型)(Ar)","W4",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041H8214","APW331防火窓 引違い窓ﾃﾗｽ戸(日射遮蔽型)","W4",null,null,null,null,null,null,"樹脂製・外窓",11,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041J1214","ﾌﾟﾗﾏｰﾄﾞIII","W4",null,null,null,null,null,null,"樹脂製・外窓",10,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041J2224","ﾌﾟﾗﾏｰﾄﾞIII (Ar)","W4",null,null,null,null,null,null,"樹脂製・外窓",7,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041K1214","ﾌﾟﾗﾏｰﾄﾞIII ﾃﾗｽﾄﾞｱ+FIX連窓","W4",null,null,null,null,null,null,"樹脂製・外窓",10,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041K2224","ﾌﾟﾗﾏｰﾄﾞIII ﾃﾗｽﾄﾞｱ+FIX連窓(Ar)","W4",null,null,null,null,null,null,"樹脂製・外窓",7,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041K3214","ﾌﾟﾗﾏｰﾄﾞIII ﾃﾗｽﾄﾞｱ","W4",null,null,null,null,null,null,"樹脂製・外窓",10,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041K4224","ﾌﾟﾗﾏｰﾄﾞIII ｾｶﾝﾄﾞﾄﾞｱ(Ar)","W4",null,null,null,null,null,null,"樹脂製・外窓",7,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041K5224","ﾌﾟﾗﾏｰﾄﾞIII ﾃﾗｽﾄﾞｱ(Ar)","W4",null,null,null,null,null,null,"樹脂製・外窓",7,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041K6224","ﾌﾟﾗﾏｰﾄﾞIII 片開きﾄﾞｱ(下部断熱腰ﾊﾟﾈﾙ仕様を除く)(Ar)","W4",null,null,null,null,null,null,"樹脂製・外窓",7,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041K7214","ﾌﾟﾗﾏｰﾄﾞIII ｾｶﾝﾄﾞﾄﾞｱ","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041T2214","APW331 木目仕様ﾃﾗｽﾄﾞｱ","W4",null,null,null,null,null,null,"樹脂製・外窓",10,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041T3224","APW331 木目仕様ﾃﾗｽﾄﾞｱ(Ar)","W4",null,null,null,null,null,null,"樹脂製・外窓",10,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041T6214","APW331 木目仕様勝手口ﾄﾞｱ中桟無","W4",null,null,null,null,null,null,"樹脂製・外窓",10,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041T7224","APW331 木目仕様勝手口ﾄﾞｱ中桟無(Ar)","W4",null,null,null,null,null,null,"樹脂製・外窓",10,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041V5224","ﾌﾟﾗﾏｰﾄﾞH 片開きドア(断熱腰ﾊﾟﾈﾙ仕様除く)(Ar) W4","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041V6224","ﾌﾟﾗﾏｰﾄﾞH ｾｶﾝﾄﾞﾄﾞｱ(断熱腰ﾊﾟﾈﾙ仕様除く)(Ar) W4","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W041Y0214","ﾌﾟﾗﾏｰﾄﾞH W4","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W041Y3214","ﾌﾟﾗﾏｰﾄﾞH ﾃﾗｽﾄﾞｱ(断熱腰ﾊﾟﾈﾙ仕様除く) W4","W4",null,null,null,null,null,null,"樹脂製・外窓",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W043L1224","ｴﾋﾟｿｰﾄﾞNEO (日射遮蔽型)(Ar)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W043L2224","ｴﾋﾟｿｰﾄﾞNEO (日射取得型)(Ar)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W043L3214","ｴﾋﾟｿｰﾄﾞNEO (日射遮蔽型)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",16,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W043M1214","ｴﾋﾟｿｰﾄﾞ・TypeS (日射遮蔽型)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",15,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W043M2224","ｴﾋﾟｿｰﾄﾞ・TypeS (日射遮蔽型)(Ar)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W043M3224","ｴﾋﾟｿｰﾄﾞ・TypeS (日射取得型)(Ar)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W043Q1224","ｴﾋﾟｿｰﾄﾞ・TypeS ﾃﾗｽﾄﾞｱ(日射取得型)(Ar)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",13,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W043Q2224","ｴﾋﾟｿｰﾄﾞ・TypeS ﾃﾗｽﾄﾞｱ(日射遮蔽型)(Ar)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W043Q3224","ｴﾋﾟｿｰﾄﾞ・TypeS 勝手口ﾄﾞｱ全面ｶﾞﾗｽﾀｲﾌﾟ(日射遮蔽型)(Ar)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",10,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W043Q4214","ｴﾋﾟｿｰﾄﾞ・TypeS 勝手口ﾄﾞｱ全面ｶﾞﾗｽﾀｲﾌﾟ(日射遮蔽型)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",14,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W043Q5224","ｴﾋﾟｿｰﾄﾞ・TypeS 勝手口ﾄﾞｱ全面ｶﾞﾗｽﾀｲﾌﾟ(日射取得型)(Ar)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W043Q6214","ｴﾋﾟｿｰﾄﾞ・TypeS 勝手口ﾄﾞｱ全面ｶﾞﾗｽﾀｲﾌﾟ(日射取得型)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",15,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W043R1224","防火窓G樹脂複合NEO (日射遮蔽型)(Ar)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W043R2224","防火窓G樹脂複合NEO (日射取得型)(Ar)","W4",null,null,null,null,null,null,"アルミ樹脂複合製・外窓",11,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W04AW1214","ﾏﾄﾞﾘﾓ 樹脂窓 北海道 W4","W4",null,null,null,null,null,null,"樹脂製・カバー(住宅用)",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W04AW3224","ﾏﾄﾞﾘﾓ 樹脂窓 北海道(Ar)片開きﾄﾞｱ 全面ｶﾞﾗｽﾀｲﾌﾟ W4","W4",null,null,null,null,null,null,"樹脂製・カバー(住宅用)",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W04AX1214","ﾏﾄﾞﾘﾓ 断熱窓 樹脂窓 W4","W4",null,null,null,null,null,null,"樹脂製・カバー(住宅用)",12,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W04BX3224","ﾏﾄﾞﾘﾓ 断熱窓 ｱﾙﾐ樹脂複合窓 ﾘﾌｫｰﾑ単体枠(Ar)樹脂ｽﾍﾟｰｻｰ W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・カバー(住宅用)",13,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W04BX4224","ﾏﾄﾞﾘﾓ 断熱窓 ｱﾙﾐ樹脂複合窓 ｼﾞｮｲﾝﾄ枠外部ｶﾊﾞｰ有(Ar) W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・カバー(住宅用)",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W04BX5224","ﾏﾄﾞﾘﾓ 断熱窓 ｱﾙﾐ樹脂複合窓 ｼﾞｮｲﾝﾄ枠外部ｶﾊﾞｰ有(Ar)樹脂ｽﾍﾟｰｻｰ W4","W4",null,null,null,null,null,null,"アルミ樹脂複合製・カバー(住宅用)",12,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W046L1115","内窓ﾌﾟﾗﾏｰﾄﾞU","W5",null,null,null,null,null,null,"樹脂製・内窓",6,null,null,null,"複層","乾燥空気"]
["窓","YKK AP株式会社","W046L2215","内窓ﾌﾟﾗﾏｰﾄﾞU Low-E","W5",null,null,null,null,null,null,"樹脂製・内窓",6,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W046L3225","内窓ﾌﾟﾗﾏｰﾄﾞU Low-E(Ar)","W5",null,null,null,null,null,null,"樹脂製・内窓",6,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W046L4145","内窓ﾌﾟﾗﾏｰﾄﾞU (真空ｶﾞﾗｽ)","W5",null,null,null,null,null,null,"樹脂製・内窓",0.2,null,null,null,"複層","真空"]
["窓","YKK AP株式会社","W04DZ0226","ｴﾋﾟｿｰﾄﾞNEO-LB[GRAF工法]","W6",null,null,null,null,null,null,"アルミ樹脂複合製・カバー(ビル用)",14,null,null,null,"Low-E複層","アルゴンガス"]
["窓","YKK AP株式会社","W04FZ1216","ｴﾋﾟｿｰﾄﾞNEO-LB[GRAF工法]防火窓","W6",null,null,null,null,null,null,"アルミ樹脂複合製・カバー(ビル用・防火仕様)",10,null,null,null,"Low-E複層","乾燥空気"]
["窓","YKK AP株式会社","W04FZ2226","ｴﾋﾟｿｰﾄﾞNEO-LB[GRAF工法]防火窓(Ar)","W6",null,null,null,null,null,null,"アルミ樹脂複合製・カバー(ビル用・防火仕様)",10,null,null,null,"Low-E複層","アルゴンガス"]

{"sheet":"検索条件","index":2,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["断熱材","ガラス","窓"]
["D1","G1","W1"]
["D2","G2","W2"]
["D3",null,"W3"]
["D4",null,"W4"]
[null,null,"W5"]
[null,null,"W6"]

{"sheet":"建具の仕様・改修方法","index":3,"n_rows":15,"n_cols":1,"rows_kept":15,"cut":false,"hidden":true,"merged":[]}
["建具の仕様・改修工法"]
["樹脂製・外窓"]
["木製・外窓"]
["アルミ樹脂複合製・外窓"]
["アルミ木複合製・外窓"]
["樹脂木複合製・外窓"]
["樹脂製・内窓"]
["木製・内窓"]
["樹脂製・カバー(住宅用)"]
["アルミ樹脂複合製・カバー(住宅用)"]
["樹脂製・カバー(ビル用)"]
["アルミ樹脂複合製・カバー(ビル用)"]
["樹脂製・カバー(ビル用・防火仕様)"]
["アルミ樹脂複合製・カバー(ビル用・防火仕様)"]
["その他の窓"]